[Date Prev][Date Next] [Chronological] [Thread] [Top]

# AVTS voting unit to card encoder: STEPS

- To: <support@gesn.com>
- Subject: AVTS voting unit to card encoder: STEPS
- From: "Lesley Thompson" <lesleytdiebold@earthlink.net>
- Date: Thu, 1 Aug 2002 19:57:31 -0500
- Organization: Diebold Election Systems, Inc.

Hello good people, can you help me out with the steps to reset an election? Thanks. Lesley HOW TO TURN A LIVE AVTS UNIT INTO A VOTER CARD ENCODER
SCENARIO 1: NO VOTES ON AVTS UNIT, USE ACTIVE ELECTION PCMCIA CARD
A. | UNSET UNIT FOR ELECTION and SET FOR CREATING VOTER ACCESS CARDS
| 1 | At the VOTING screen, insert MANAGER CARD
| 2 | Input PASSWORD and press OK button
| 3 | Press DONE REPORTING button
|  | (NOTE: zero report should have already been printed and counter should still be at 0)
| 4 | At the POST ELECTION screen, insert MANAGER CARD again
| 5 | Input PASSWORD and press OK button
| 6 | At the MODE screen, press RESET TO PRE-ELECTION MODE button
| 7 | Press EXIT ADMINISTRATOR button
| 8 | At the ELECTION MANAGEMENT screen, press CREATE VOTER CARDS
| 9 | Begin creating cards
|  | NOTE: This ACTIVE ELECTION PCMCIA Card will not be accumulated with the other units unless after the polls close you SET FOR ELECTION and then END THE ELECTION and PRINT FINAL REPORT.
B. | RESET UNIT FOR ENDING ELECTION and PRINTING FINAL REPORT
| 1 | At the CREATE CARDS screen, press EXIT.
| 2 |
| 3 |
| 4 |
| 5 |
| 6 |
| 7 |
| 8 |
| 9 |

- Follow-Ups:
  - Re: AVTS voting unit to card encoder: STEPS
    - From: "Tari Runyan" <tarir@dieboldes.com>

- Prev by Date: Converting audio files into MP3 format under Windows XP
- Next by Date: Re: AVTS voting unit to card encoder: STEPS
- Index(es):
  - Chronological
  - Thread