[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: OS and TS upload

- To: <support@gesn.com>
- Subject: RE: OS and TS upload
- From: "Lisa Martin" <lisam@gesn.com>
- Date: Fri, 28 Jun 2002 13:25:27 -0500
- Importance: Normal
- In-reply-to: <000001c21ecf$4ee96f60$2304a8c0@kclark>

I believe Don is asking this on behalf on Jefferson County, KY, who wants to do this for the upcoming November election. They will have one polling place, a Center for the Blind, where the visually impaired voters will be voting. They only bought 4 touch screens specifically for this purpose. Only the visually impaired voters will be allowed to vote on the TS, but as other, non-visually impaired voters are assigned to that precinct, they will have to vote on the OS since the voters in all other precincts will be voting on the OS. Jefferson County has concerns about everything working smoothly if they are transferring results from both OS and TS at the same time, which they insist on. They want to be trained on the appropriate way to integrate both systems by the end of July, and they want to see it work before they do it. Lisa Martin Diebold Election Systems (800)433-8683 (c) (469) 667-6215 -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ken Clark Sent: Friday, June 28, 2002 1:12 PM To: support@gesn.com Subject: RE: OS and TS upload Don, there are no “present procedures” on this as of yet, since I don’t think anyone has done this in anything but a small test capacity yet. Mark, your setup will indeed work. Hats off for intuiting the process. We of course thought about this possibility the day we started work on AVTS integration with GEMS several years ago. We had kinda hoped (faintly) that no one would be actually crazy enough to do it though. Right now the vote center dialog allows you to specify the count method for a vote center, and the number of memory cards. What we would need to do to do this right is to allow the user to specify for the vote center not a single count method, but multiple count methods. Our data structures don’t support this at the moment, so it is not a trivial change unfortunately. Mark’s setup will have to suffice for the interim. Could one or both of you write up some background on why they want to do this? My main worry is that we can’t possibly make enough money supporting such a complicated configuration. It is basically the worst of both worlds. Don’t get me wrong, GEMS can do it. I just wonder out loud whether this is even something we want to be offering customers. I guess this is an executive committee thing to answer. Ken -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com] On Behalf Of Mark S Earley Sent: Wednesday, June 26, 2002 12:32 PM To: support@gesn.com Subject: RE: OS and TS upload I need clarification on this also, as most of the Florida counties eventually want one TS and one OS in each precinct. My understanding was that you would create an AVOS memory card and an AVTS memory card for each report precinct – the hard part is doing that. See attached test database for my attempt at this. While the method was not intuitive, I think I managed to build something that would work by making a separate Counter Group (each with its own Vote Center Type) for the OS precinct machines and the TS precinct machines. My question is would the results from each set of machines (OS and TS) add correctly for each of the reporting precincts? Also, my understanding is that you would need one set of modem ports for AVOS upload and one set of modem ports for AVTS upload. Each set of ports would have its own rollover phone number. The AVTS ports would also be configured for RAS. Is this the way to do it? All of this is just speculation based upon trial and error this past hour. I have not actually downloaded or uploaded any cards or results. Mark Earley 850 422-2100 - office/fax 850 322-3226 - cell -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Don Bizmaier Sent: Wednesday, June 26, 2002 2:21 PM To: support@gesn.com Subject: OS and TS upload Can anyone tell me what the present procedures are for uploading results when both OS and TS units are used? I have heard both ways - that they can upload at the same time and that they cannot. If they cannot it is going to be a real problem as juridiction start to use at least one TS in each polling place, which is what many OS customers are looking to do in the future. Thanks: Don Donald W. Biszmaier Support Services Specialist Diebold Election Systems, Inc. 7717 Greenwood Rd. Louisville, Ky. 40258 Office 502-244-8645 Cell 502-314-6936 Fax 502-254-7835

- References:
  - RE: OS and TS upload
    - From: "Ken Clark" <ken@gesn.com>

- Prev by Date: RE: OS and TS upload
- Next by Date: Re: charging indicator on R6 running 4-3-9
- Index(es):
  - Chronological
  - Thread