[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: PLEASE REVIEW & COMMENT: JoCoKs AVOS Central Count Scanner Diagonstics Checklist

- To: <support@dieboldes.com>
- Subject: RE: PLEASE REVIEW & COMMENT: JoCoKs AVOS Central Count Scanner Diagonstics Checklist
- From: "Steve Knecht" <stevek@dieboldes.com>
- Date: Mon, 5 Aug 2002 21:27:36 -0700
- Importance: Normal
- In-reply-to: <006201c22d01$fbb49bd0$63e2fea9@PERSONAL>

> Once I'd tested the scanner I wouldn't go into diagnostic mode. You've got a good chance that someone will accidentally change the settings. I would not follow the procedures you've set out. Sorry for the late response but I was on vacation. I think you improve the chance of screwing up the system settings. Plus, these are pretty much weeds in the forest relative to central count. -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Lesley Thompson Sent: Tuesday, July 16, 2002 12:50 PM To: support@gesn.com Subject: PLEASE REVIEW & COMMENT: JoCoKs AVOS Central Count Scanner Diagonstics Checklist Dear fellow support staff, below is Johnson County's current checklist for AVOS scanner diagnostics prior to central count. I need this reviewed to make sure it includes all the diagnostic type items that need to be tested. Thanks in advance for any and all help granted. Lesley Lesley Koop Thompson Customer Service Project Manager Diebold Election Systems, Inc. lesley@dieboldes.com OR lesleytdiebold@earthlink.net 512-413-7618 (cell) 415-235-6553 (DESI cell)
> Election Date: | Scanner Number:
> JoCoKs Scanner Diagnostics Checklist – AccuVote-OS Central Count
> Night Before
> | Turn on scanner to charge battery – leave on overnight
> # Test Day
> | Turn scanner off
> | Check that printer has sufficient paper – Replace paper roll with AccuVote off
> | Turn on Feeder
> | Hold down Y & N buttons while turning AccuVote on Release when display comes up Scanner is now in Diagnostics Mode
> | # Test Network? – Y
> | · Set Baud rate to 9600? – N
> | · Set Baud rate to 19200? – Y
> | Logging In Message
> | Connecting Message
> | · Echo Connection Test? – N
> | · Test Network – N
> | # Test LCD Display? – Y
> | · Test Continuous? – N
> | # Test System Memory? - Y
> | · Test Continuous? – N
> | Test Printer? UNPLUG power from AccuVote and Feeder, then – Y (Low Power message will flash while unplugged – this is OK)
> | · Repeat Test – Y (total of 3 tests)
> | Check tape for legible output
> | Plug power back in
> | · Repeat Test – N
> | # Test Main Serial Port? – N
> | # Test Auxiliary Serial Port? – N
> | Test Ballot Deflector? – N
> | Test Ballot Reader – Y
> | · Test with Auto feeder? – Y
> | Insert Diagnostic Ballot in Reader – run card through four times – on the 5th time, hold down Y to get report
> | · Turn ballot over & repeat on other side
> | (Each report will show number of ballots read, length = 41, % of values – look for 100% and 0% on each test)
> | Turn AccuVote and Feeder OFF
> | Check for sufficient paper – replace if necessary
> | Replace ribbon if necessary
> Tested by: | Date:

- Follow-Ups:
  - Re: PLEASE REVIEW & COMMENT: JoCoKs AVOS Central Count Scanner Diagonstics Checklist
    - From: "Don Bizmaier" <donaldb@dieboldes.com>

- Prev by Date: Fw: WCE 300 - July 05, 2002 Release
- Next by Date: Re: PLEASE REVIEW & COMMENT: JoCoKs AVOS Central Count Scanner Diagonstics Checklist
- Index(es):
  - Chronological
  - Thread