[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: VIBS Voter Card Encoding Problem?

- To: <support@gesn.com>
- Subject: RE: VIBS Voter Card Encoding Problem?
- From: "Ken Clark" <ken@gesn.com>
- Date: Fri, 14 Jun 2002 21:53:47 -0800
- Importance: Normal
- In-reply-to: <005901c213bf$268c37c0$0203a8c0@desktop>

Thanks for everyone’s input on this topic. The new behavior for the * key is as follows: No. * Key Presses Display Ballot not pressed [nothing] normal ballot first M magnified ballot second VM VIBS ballot, magnified third VH VIBS ballot, hidden There is no lone V, which would be VIBS but not magnified. This will be in Voter Card Encoder 1.1.3. Note the name change from Card Manager with this release, to go with the unit’s new suit. See attached. Ken

Attachment: `label.jpg`
Description: JPEG image

- Follow-Ups:
  - Re: VIBS Voter Card Encoding Problem?
    - From: "Tari Runyan" <tarir@gesn.com>

- References:
  - Re: VIBS Voter Card Encoding Problem?
    - From: "Steve Knecht" <stevek@gesn.com>

- Prev by Date: RE: Puerto Rico - Modems Hanging after first data transfer
- Next by Date: Re: VIBS Voter Card Encoding Problem?
- Index(es):
  - Chronological
  - Thread