[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: R6 Power status

- To: <support@gesn.com>
- Subject: Re: R6 Power status
- From: "Talbot Iredale" <tiredale@gesn.com>
- Date: Thu, 7 Jun 2001 09:18:20 -0700
- References: <PPECJKNKLDJLKJPKPPIOOEKPCOAA.ken@gesn.com> <002301c0ef0a$30c37080$a5dffc9e@default>

    Steve,

        The current R6 unit does not yet have the battery charge status yes
    implements.  Therefore the current system will display the following:

    Charging - If it has AC power and the battery is not at full voltage.
    High: If does has AC power and the battery is at full voltage.
    Low: If does not have AC power.

    Tab

    ----- Original Message -----
    From: "Steve Knecht" <skglobal@earthlink.net>
    To: <support@gesn.com>
    Sent: Wednesday, June 06, 2001 9:27 PM
    Subject: Re: R6 Power status

    > Dear Big Bucks,
    >
    > During the day in Chico on Tuesday, I setup the R6 and charged battery
    until
    > it said "high".  And I kept charging it for another 1/2 hours or so.   I
    > then unplugged it for about 3 minutes and it went to "low".  I don't have
    a
    > problem with the definitiions at all.  High is High.  Low is Low.  After
    > all, English is the language of Science all over the world. However, if
    High
    > is so transitory, like any good high, then perhaps we could call it "Quick
    > High" or "Flash High" or "Don't-Blink-An-Eye High".
    >
    > It does beg the question regarding how long these ontological battery
    states
    > of  existence should last.  Do I have a "prototype" battery too?
    >
    > Still Wondering and Wandering in Chico
    >
    > ----- Original Message -----
    > From: Ken Clark <ken@gesn.com>
    > To: <support@gesn.com>
    > Sent: Tuesday, June 05, 2001 9:43 AM
    > Subject: RE: R6 Power status
    >
    >
    > > > From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf
    Of
    > > > Tyler Lincks
    > > >
    > > > The "Power" field on the R6 election mode screen can (according to the
    > R6
    > > > User's Guide) be defined as high,
    > >
    > > The charge in the battery is high.
    > >
    > > > low,
    > >
    > > The charge in the battery is low.
    > >
    > > > critical,
    > >
    > > The charge in the battery is critically low.
    > >
    > > > charging,
    > >
    > > The battery is charging.
    > >
    > > > no battery,
    > >
    > > There is no battery.
    > >
    > > > and
    > > > unknown.
    > >
    > > The state of the battery isn't known.
    > >
    > > > What does each of these mean?
    > >
    > > That's why they pay us the big bucks, to explain these things.
    > >
    > > Ken
    > >

- Follow-Ups:
  - Re: R6 Power status
    - From: "Steve Knecht" <skglobal@earthlink.net>

- References:
  - RE: R6 Power status
    - From: "Ken Clark" <ken@gesn.com>
  - Re: R6 Power status
    - From: "Steve Knecht" <skglobal@earthlink.net>

- Prev by Date: Re: R6 Power status
- Next by Date: RE: R6 Power status
- Index(es):
  - Chronological
  - Thread