[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: VIBS with Spyrus on non-Vibs R4

- To: <bugtrack@dieboldes.com>
- Subject: Re: VIBS with Spyrus on non-Vibs R4
- From: "Greg Forsythe" <gfglobal@earthlink.net>
- Date: Thu, 25 Oct 2001 16:01:51 -0400
- References: <PPECJKNKLDJLKJPKPPIOCEBPDDAA.ken@dieboldes.com>

----- Original Message ----- From: Ken Clark To: bugtrack@dieboldes.com Sent: Thursday, October 25, 2001 3:29 PM Subject: RE: VIBS with Spyrus on non-Vibs R4 I can't reproduce the problem yet. Two questions: Does the problem only occur when creating VIBS cards with Spyrus, NO - or do VIBS cards created with ballot station also exhibit the problem.YES Does the problem occur in test count no voter card, selecting the VIBS checkbox. YES It appears that Spyrus has nothing to do with the condition. Anytime VIBS is selected with this non VIBS R4, and the error is answered with OK, the next normal voter card brings the screens up in magnify mode and will not reset. The only way out is Ctl, Alt, Del. Ken -----Original Message----- From: owner-bugtrack@dieboldes.com [mailto:owner-bugtrack@dieboldes.com]On Behalf Of Greg Forsythe Sent: Thursday, October 25, 2001 11:19 AM To: bugtrack@dieboldes.com Subject: Re: VIBS with Spyrus on non-Vibs R4 ----- Original Message ----- From: Ken Clark To: bugtrack@dieboldes.com Sent: Thursday, October 25, 2001 1:36 PM Subject: RE: VIBS with Spyrus on non-Vibs R4 From: owner-bugtrack@dieboldes.com [mailto:owner-bugtrack@dieboldes.com]On Behalf Of Greg Forsythe Sent: Thursday, October 25, 2001 10:36 AM BSNT-4-1-2 non VIBS R4, GEMS-1-18-4-1, CM-0-2-10 Election mode Select asterisk on Spyrus to create VIBS card. Caution appears when voter card has been read. What is the caution? The following error has been detected: Error initializing VGroup Select Dlg Failed to find data OK Touch OK and election screen with flag appears. Insert a non VIBS voter card. Instructions and following screens are magnified voter card after voter card. The only way back to a regular screen is the three fingered salute, re-boot, (I tried WD-40 and it didn't fix it). Can you reproduce all this? Tried two different Spyrus with same results. Please send me the .gbf file for your database directly. Attached Is this a VIBS database, or not? The database I have is not, however Cathi's comments As you are probably aware, there are two cities hosting the TS demo elections. Here are the databases being used for the GA elections. However, as indicated below, they have been sent to the Omaha office for VIBS modification. After the databases were pretty much already done, the SOS in GA decided they wanted the vendors to provide a VIBS unit in each city. I don't have the equipment to do this so that is why the DB's were sent to Omaha. Question: Will a voter card programmed VIBS with a Spyrus inserted into a non VIBS R6 cause the same condition? There is no such thing as a "non VIBS R6". They are all the same units. Only difference is they keypad and headphones plugged in, and the software isn't actually aware that they are in fact plugged in. As to whether it behaves the same on NT as on CE, I have no idea, but I would suspect the answer is yes. Please try to get yourself an R6 as soon as one becomes available. You are important to the testing effort. In the mean time, some one in support will need to be assigned to test your database for you. If there is one VIBS out of 4 or 5 R6s in a voting location and the voter puts a VIBS card into a non VIBS R6 will that R6 have to be re-booted? Again, there is no such thing as a non-VIBS R6. Thank you, did not know. Ken

- Follow-Ups:
  - RE: VIBS with Spyrus on non-Vibs R4
    - From: "Ken Clark" <ken@dieboldes.com>

- References:
  - RE: VIBS with Spyrus on non-Vibs R4
    - From: "Ken Clark" <ken@dieboldes.com>

- Prev by Date: RE: VIBS with Spyrus on non-Vibs R4
- Next by Date: RE: BS 4-1-1-0 Summary Screen not returning to correct candidate position
- Index(es):
  - Chronological
  - Thread