[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: Touch Screen Calibration with BS Software

- To: <rcr@dieboldes.com>
- Subject: RE: Touch Screen Calibration with BS Software
- From: "Ian S. Piper" <ian@dieboldes.com>
- Date: Wed, 24 Oct 2001 11:34:46 -0500
- Importance: Normal
- In-Reply-To: <NDBBJBKEHMHBEPDMLKOLAEPKDEAA.ljdglobal@dieboldes.com>

Q: How would you select an "ELO Calibration" button using the touch screen when the calibration is out to begin with? Q: Could a keyboard be used to select this function, if the touch screen is so far out of calibration that it can't be selected by using the touch screen? Ian -----Original Message----- From: owner-rcr@dieboldes.com [mailto:owner-rcr@dieboldes.com]On Behalf Of Larry Dix Sent: October 24, 2001 11:06 AM To: Rcr@Gesn. Com Subject: Touch Screen Calibration with BS Software Allow a user to do the touch screen calibration from within ballot station software. With the ultimate goal of locking users out of the OS, can a call be made to the ELO executable so that it accessed from the System Setup - Diagnostics Larry J. Dix Vice President of Operations Global Election Systems

- Follow-Ups:
  - RE: Touch Screen Calibration with BS Software
    - From: "Ken Clark" <ken@dieboldes.com>
  - Re: Touch Screen Calibration with BS Software
    - From: "Steve Knecht" <skglobal@earthlink.net>

- References:
  - Touch Screen Calibration with BS Software
    - From: "Larry Dix" <ljdglobal@dieboldes.com>

- Prev by Date: RE: Touch Screen Calibration with BS Software
- Next by Date: RE: Touch Screen Calibration with BS Software
- Index(es):
  - Chronological
  - Thread