[Date Prev][Date Next] [Chronological] [Thread] [Top]

# 128mb PCMCIA Cards - battery low error

- To: "Support Team" <support@gesn.com>
- Subject: 128mb PCMCIA Cards - battery low error
- From: "Jeff Hintz" <jhglobal@earthlink.net>
- Date: Wed, 2 Jan 2002 15:54:50 -0600
- Importance: Normal

When you insert the new 128 MB PCMCIA cards it gives you the following message: Warning: Battery power may not be sufficient to run your PC card. Some PC cards, such as modem cards, require AC power. If you choose Yes below, you may want to save any work in progress. Do you want to use this PC card on battery power? Yes No Why does this message come up? What is the correct answer to this question? You do not get the message if the card is inserted before the machine is turned on. Should the card be inserted first or is there more to the message than that? Jeff

- Follow-Ups:
  - RE: 128mb PCMCIA Cards - battery low error
    - From: "Steve Ricke" <steve@gesn.com>
  - Sacramento demo database
    - From: Robert Chen <chenrob@pacbell.net>

- Prev by Date: Re: confusion about back plates and reports in 1-17-20
- Next by Date: RE: 128mb PCMCIA Cards - battery low error
- Index(es):
  - Chronological
  - Thread