[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Fw: AccuVote Server 1 - Happy Faces

- To: <support@gesn.com>
- Subject: Fw: AccuVote Server 1 - Happy Faces
- From: "Steve Knecht" <skglobal@earthlink.net>
- Date: Thu, 17 Feb 2000 17:50:45 -0800

The issue here is that I'm told we've made no changes to GEMS in this area, but here is what Mike and I did. We created a small db in 1.11.2. created db loaded memory uploaded memory card with the following lights Yelllow HF (Happy Face) Modem On-line Green HF Connected Yellow HF AccuVote On-line (AccuVote still connected Yellow HF Modem Online (ended up here after cycling after AV turned off) This is the way it worked in 1.11.2. We then upgraded the DB to 1.14.8 and Reset Election downloaded new memory card uploaded the memory card The following message shows what the Server status and the differences of the server console. Point: the ONLY change is in GEMS. Same modems, same memory card, same AccuVote, same phone line. Even though development is saying no changes are made to GEMS in this area, something in GEMS is different. Question: What Mike and I notice is differenct is the upload console, or that seems the major change. Would the changes made to the upload console have any affect on the modem signal handling. Specifically, Fresno is no longer able to even upload two in a row on their modem boxes. Looking for answers. I have attached both the .dbf files (one in 1.11.2 and one in 1.14.8) Yellow HF Modem On-line Green HF Connected Upload ) Yellow HF AccuVote On-line (until AccuVote turned off) Green HF Connected Green HF Connected -----Original Message----- From: Steve Knecht <skglobal@earthlink.net> To: bugtrack@gesn.com <bugtrack@gesn.com> Date: Thursday, February 17, 2000 4:08 PM Subject: AccuVote Server 1 - Happy Faces It has taken an hour or so to get the following sequence, but here it is.... In Rev. 1.14.8 after an upload (starting clean with yellow smiley face and Modem On-line) the Server under the Port Tab goes thru the following sequence: Yellow Modem Ready (to start) Green Connected Upload (modem answers and data is uploaded) Green Connected (when Results sent OK, Turn unit off) Red Off-line (some part of cycling) Yellow AccuVote On-line (until AV is shutoff and CD is lost) Green Connected (Stays until next call to modem) goes to disconnected on next ring of phone.... Red off-line disconnected (Briefly when next call hits modem) Yellow AccuVote On-line (very fast blip) Green connected upload (next data upload begins) If you begin an upload with the Yellow happy face, and green is supposed to connote a connection and data loading, is this a bug that the system doesn't go back to yellow Modem ready, when the AccuVote is turned off and the next call comes in. It still loads, but it is confusing most customers when the light stays green and says connected at pretty much all times. Maybe this is RCR, I don't know.

Attachment: `test modem v1.14.8.dbf`
Description: Binary data

Attachment: `test modem v1-11-2.dbf`
Description: Binary data

- Follow-Ups:
  - RE: AccuVote Server 1 - Happy Faces
    - From: "Ken Clark" <ken@gesn.com>

- Prev by Date: Re: installation diskettes
- Next by Date: FW: 1-14-8 CC -decks lost in central count window - so unable to clear
- Index(es):
  - Chronological
  - Thread