[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: Touch Screen Calibration with BS Software

- To: <rcr@dieboldes.com>
- Subject: RE: Touch Screen Calibration with BS Software
- From: "Ken Clark" <ken@dieboldes.com>
- Date: Wed, 24 Oct 2001 10:19:36 -0700
- Importance: Normal
- In-Reply-To: <NEBBIDEKLMNCHGCGIFJCMEEECFAA.steve@dieboldes.com>

In the new calibration procedure, you have to press the three calibration points twice in succession, with each try being within a small error factor of the previous. You might accidentally miss a button once, but not twice, and certainly not twice the same way. If you show me the specs, we can probably even throw out "that can't be right" calibration input from users. Take a look at a palm pilot some day. It doesn't have a keyboard. It does have touch screen calibration. Ken -----Original Message----- From: owner-rcr@dieboldes.com [mailto:owner-rcr@dieboldes.com]On Behalf Of Steve Ricke Sent: Wednesday, October 24, 2001 10:19 AM To: rcr@dieboldes.com Subject: RE: Touch Screen Calibration with BS Software During the calibration procedure it is possible to touch the screen away from the calibration targets thus throwing calibration off to a point of no return. Keyboard navigation to return to the calibration function is the only recourse in this situation. -----Original Message----- From: owner-rcr@dieboldes.com [mailto:owner-rcr@dieboldes.com]On Behalf Of Ken Clark Sent: Wednesday, October 24, 2001 11:50 AM To: rcr@dieboldes.com Subject: RE: Touch Screen Calibration with BS Software Keyboard navigation probably makes some sense for the administrative functions: tab through buttons, space to press button, etc. But before we get in a knot about this, just how far out of calibration can these things really get on their own before we just declare the touch screen broken? I mean, its a big button, and you can always use some smarts and touch a little to the left or right based on feedback. If the screen is going out of calibration to the point that this technique doesn't work, something is seriously wrong. Show me the specs. Ken -----Original Message----- From: owner-rcr@dieboldes.com [mailto:owner-rcr@dieboldes.com]On Behalf Of Ian S. Piper Sent: Wednesday, October 24, 2001 9:35 AM To: rcr@dieboldes.com Subject: RE: Touch Screen Calibration with BS Software Q: How would you select an "ELO Calibration" button using the touch screen when the calibration is out to begin with? Q: Could a keyboard be used to select this function, if the touch screen is so far out of calibration that it can't be selected by using the touch screen? Ian -----Original Message----- From: owner-rcr@dieboldes.com [mailto:owner-rcr@dieboldes.com]On Behalf Of Larry Dix Sent: October 24, 2001 11:06 AM To: Rcr@Gesn. Com Subject: Touch Screen Calibration with BS Software Allow a user to do the touch screen calibration from within ballot station software. With the ultimate goal of locking users out of the OS, can a call be made to the ELO executable so that it accessed from the System Setup - Diagnostics Larry J. Dix Vice President of Operations Global Election Systems

- Follow-Ups:
  - RE: Touch Screen Calibration with BS Software
    - From: "Ian S. Piper" <ian@dieboldes.com>

- References:
  - RE: Touch Screen Calibration with BS Software
    - From: "Steve Ricke" <steve@dieboldes.com>

- Prev by Date: RE: Touch Screen Calibration with BS Software
- Next by Date: RE: Touch Screen Calibration with BS Software
- Index(es):
  - Chronological
  - Thread