[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: Blackhawk, IA 11/06/01 election 194F

- To: <support@gesn.com>
- Subject: RE: Blackhawk, IA 11/06/01 election 194F
- From: "Cathy Colgan" <cacglobal@earthlink.net>
- Date: Mon, 29 Oct 2001 15:24:41 -0600
- Importance: Normal
- In-reply-to: <NEBBIDEKLMNCHGCGIFJCOEFJCFAA.steve@gesn.com>

Blackhawk, Ia 194F! -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Steve Ricke Sent: Monday, October 29, 2001 3:21 PM To: support@gesn.com Subject: RE: Blackhawk, IA 11/06/01 election 194F 1.94F can be the equivalent firmware to just about any 1.94(choose a letter) firmware. The key is the character after the F: +,#,<,&,etc. . This was done due to certification issues. Please let me know what that character is so we can tell what it is equivalent to. You can look it up on the ROM EQUIVALENCE chart at: http://staff.gesn.com/resources/avos/relnotes -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Global Chouteau Sent: Monday, October 29, 2001 2:10 PM To: support@gesn.com Subject: Re: Blackhawk, IA 11/06/01 election 194F This is a "version" of the "long mark" condition that M. Shamus (sp?) was so fond of..."High Ovals" (excessively so) can cause "black blindness" before the reader reaches the "hot spot area".. That is why feeding the ballots bottom first is an assist............The new design (visible light) are not affected by black blindness............ ----- Original Message ----- From: Cathy Colgan To: support@gesn.com Sent: Monday, October 29, 2001 1:12 Aftrnoon Subject: RE: Blackhawk, IA 11/06/01 election 194F i found some ballots where the reg "tic marks" looked good but lining up oval with ruler shows them "high" charlie conrad confirms that "high" ovals are not good that is why "okay" when feeding ballots bottom first. I have told her to start with fresh "test ballots and new pen and let me know. i have explained the "high" oval situation in infra red readers and if her tests come out satisactorily she will have her poll workers feed bottom up if error messages. hopefully that is all there is. thanks -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Greg Forsythe Sent: Monday, October 29, 2001 9:39 AM To: support@gesn.com Subject: Re: Blackhawk, IA 11/06/01 election 194F . > > Visible light machine test OK on all ballots. Then you know the ballots work! > > Infra red using same test ballots as VL - Fully voted ballot some undefined Undef is the same as Invalid Mark. It's on the cusp, neither a mark nor fly speck. Not enugh carbon in the mark. > races some races showing blank. showing some okay in 4 ballot directions but > some blanks candidates. It is hit and miss on variance depending on > orientation. Not enough carbon in the mark. Inconsistent. Get new pens. Use a Sharpie for testing. Check the printing. > > always errors when head first (back and front) always ok when ballot upside > down (front and back) You are using different sensors when you reverse the ballot. Use a Sharpie and you will see > > Using eberhard faber pen 60110. had election october 2 - no problem in test > or election. The carbon may be used up in these pens. Get new or unused Eberhard Faber 60110 pens. > > I had her send sample ballots i am getting same hit and miss results. With a Sharpie? If they work OK in VL they should work in IR > >

- Follow-Ups:
  - RE: Blackhawk, IA 11/06/01 election 194F
    - From: "Steve Ricke" <steve@gesn.com>

- References:
  - RE: Blackhawk, IA 11/06/01 election 194F
    - From: "Steve Ricke" <steve@gesn.com>

- Prev by Date: RE: Blackhawk, IA 11/06/01 election 194F
- Next by Date: RE: Blackhawk, IA 11/06/01 election 194F
- Index(es):
  - Chronological
  - Thread