[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: WinCE 3.00 June 7th Release

- To: <support@gesn.com>
- Subject: RE: WinCE 3.00 June 7th Release
- From: "Ken Clark" <ken@gesn.com>
- Date: Fri, 14 Jun 2002 10:15:57 -0800
- Importance: Normal
- In-reply-to: <00f101c213c6$6329c790$1404a8c0@TIredale>

What happens if you put the epboot.nb0 file on the PCMCIA card with the fboot.nb0 and nk.bin file? Ken -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com] On Behalf Of Talbot Iredale Sent: Friday, June 14, 2002 9:11 AM To: support@gesn.com Subject: Re: WinCE 3.00 June 7th Release The epboot.nb0 file is used to create the EPROMS which are used during initialial production. I have included these in the zip file so all the files for this release are kept together. Tab ----- Original Message ----- From: Ken Clark To: support@gesn.com Sent: Friday, June 14, 2002 11:05 AM Subject: RE: WinCE 3.00 June 7th Release What is the epboot.nb0 file? Why don’t we need it? Why would we need it? How is it different from the fboot.nb0 file? Ken -----Original Message----- From: owner-sw-announce@gesn.com [mailto:owner-sw-announce@gesn.com] On Behalf Of Talbot Iredale Sent: Thursday, June 13, 2002 3:57 PM To: Software Announcements Subject: WinCE 3.00 June 7th Release The new WinCE 3.00 and bootloader are on the ftp site. The file is WCE300-020607.zip and the password is "idns84jdb712f". Note: Coy the fboot.nb0 and nk.bin files to a pcmcia card and install in the bottom slot of the AVTS unit and the turn the system on. You do not need the epboot.nb0 file. Tab

- Follow-Ups:
  - RE: WinCE 3.00 June 7th Release
    - From: "Ian S. Piper" <ian@gesn.com>
  - Re: WinCE 3.00 June 7th Release
    - From: "Talbot Iredale" <tiredale@gesn.com>

- References:
  - Re: WinCE 3.00 June 7th Release
    - From: "Talbot Iredale" <tiredale@gesn.com>

- Prev by Date: RE: VIBS Voter Card Encoding Problem?
- Next by Date: RE: WinCE 3.00 June 7th Release
- Index(es):
  - Chronological
  - Thread