[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: Port Server II setup

- To: <support@gesn.com>
- Subject: RE: Port Server II setup
- From: "Ken Clark" <ken@gesn.com>
- Date: Tue, 6 Jul 1999 09:48:10 -0500
- Importance: Normal
- In-reply-to: <NCBBIGGNCKBDKCCGPEOACEELCLAA.ken@gesn.com>

Jeff Hallmark points out there is a missing parameter to the "set user" command: password=off. So, the whole thing becomes: Set config ip=xxx.xxx.xxx.xxx set forwarding state=passive proxyarp=on set ippool count=16 ip=xxx.xxx.xxx.xxx set user name=accuvote protocol=ppp mtu=1500 ipaddr=ippool pppauth=none defaultaccess=netservice netservice=on compression=vj password=off set line baud=19200 range=1-16 set flow altpin=on range=1-16 Ken -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ken Clark Sent: Tuesday, June 29, 1999 10:38 AM To: support@gesn.com Subject: FW: Port Server II setup Below is an old email I wrote describing how to set up the Port Server II for central count. I won't claim it is strictly correct (I never got a reply to the mail when I sent it), but for now it is the closest thing we have to a Port Server setup document. Ken -----Original Message----- From: owner-devel@ns.gesn.com [mailto:owner-devel@ns.gesn.com]On Behalf Of Ken Clark Sent: Friday, August 07, 1998 4:38 PM To: devel@gesn.com Cc: nel@gesn.com Subject: Port Server II setup Okay, though some help from Guy and some guessing, I now have my port server running. Here are the commands I issued to the port server. I don't know if this is a minimal set, or if I missed something, but it seems to work. This "example" should be incorporated into whatever documentation we are writing for this. Let me know if this looks okay. One thing that looks a bit suspicious to me is the mtu. set config ip=192.168.3.104 set forwarding state=passive proxyarp=on set ippool count=16 ip=192.168.3.111 set user name=accuvote protocol=ppp mtu=1500 ipaddr=ippool pppauth=none defaultaccess=netservice netservice=on compression=vj set line baud=19200 range=1-16 set flow altpin=on range=1-16 ---------------------------------------------------------- Ken Clark Global Election Systems Don't anthropomorphize computers. They don't like that.

- Prev by Date: RE: AVTS software and Win98
- Next by Date: AVTS - Diagnostics & Installation
- Index(es):
  - Chronological
  - Thread