[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: Touch Screen Calibration with BS Software

- To: <rcr@dieboldes.com>
- Subject: RE: Touch Screen Calibration with BS Software
- From: "Ken Clark" <ken@dieboldes.com>
- Date: Wed, 24 Oct 2001 11:01:01 -0700
- Importance: Normal
- In-Reply-To: <042301c15cb5$aad61f80$3c03a8c0@obrien>

From: owner-rcr@dieboldes.com [mailto:owner-rcr@dieboldes.com]On Behalf Of Ian S. Piper Sent: Wednesday, October 24, 2001 11:00 AM It would be interesting to know how the palm pilot handles mis-calibrations and factory setups. They might do it through software controls or they may have some interface port that allows for an alternate input device. No; they use the proceedure I described: double entry. If you screw up twice, you are deemed too stupid to own a palm pilot. Then you remove the batteries and get factory defaults, and start over. My understanding, from Tab's explanation of the magic PCMCIA card, is that the system would boot and operate from the image on that card. Would this magic PCMCIA card allow changes to the "Internal Flash Filesystem"? Yes, but lets not wade too deep here, okay. Ken

- Follow-Ups:
  - RE: Touch Screen Calibration with BS Software
    - From: "Ian S. Piper" <ian@dieboldes.com>

- References:
  - RE: Touch Screen Calibration with BS Software
    - From: "Ian S. Piper" <ian@dieboldes.com>

- Prev by Date: RE: Touch Screen Calibration with BS Software
- Next by Date: Re: Touch Screen Calibration with BS Software
- Index(es):
  - Chronological
  - Thread