[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: 128mb PCMCIA Cards - battery low error

- To: <support@gesn.com>
- Subject: Re: 128mb PCMCIA Cards - battery low error
- From: "Talbot Iredale" <tiredale@gesn.com>
- Date: Wed, 9 Jan 2002 13:56:59 -0800
- References: <00b401c197af$f5763400$3c03a8c0@obrien>

This message should only popup if there is no AC power present. I have removed this message from the WinCE 3.0 version that we will be releasing soon, since the battery in the AVTS unit is sufficiently powerful enough to drive all of the supported cards. Tab ----- Original Message ----- From: Ian S. Piper To: support@gesn.com Sent: Monday, January 07, 2002 11:17 AM Subject: RE: 128mb PCMCIA Cards - battery low error Steve: Please be aware that your conclusions as to the event trigger are mistaken. If AC is plugged into a unit, Windows CE 2.12, at present, is oblivious to any battery capacity test that the PIC is performing. Please read the theory of operation for the PIC code for a detailed explanation. The reason for this message popping up is unknown. Sincerely, Ian S. Piper -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Steve Ricke Sent: January 02, 2002 5:03 PM To: support@gesn.com Subject: RE: 128mb PCMCIA Cards - battery low error This is a Windows CE message. This will happen if you insert any PCMCIA card during the first 130 seconds after power-up. The system is on battery power during this time to evaluate the battery charge level. Likewise, it will also occur any time the card is inserted without AC applied. It will not affect the operation of the unit if a card is inserted during this condition. Cards inserted before turning on the power will not generate this message. It does not matter whether it is running on the battery or if AC is applied. Cards inserted after 130 seconds with AC power applied will not generate this message. It is OK to answer "Yes" when the system asks if you want to use the card on battery power. Steve R. -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Jeff Hintz Sent: Wednesday, January 02, 2002 3:55 PM To: Support Team Subject: 128mb PCMCIA Cards - battery low error When you insert the new 128 MB PCMCIA cards it gives you the following message: Warning: Battery power may not be sufficient to run your PC card. Some PC cards, such as modem cards, require AC power. If you choose Yes below, you may want to save any work in progress. Do you want to use this PC card on battery power? Yes No Why does this message come up? What is the correct answer to this question? You do not get the message if the card is inserted before the machine is turned on. Should the card be inserted first or is there more to the message than that? Jeff

- References:
  - RE: 128mb PCMCIA Cards - battery low error
    - From: "Ian S. Piper" <ian@gesn.com>

- Prev by Date: TSText Files - Where are control points?
- Next by Date: RE: TSText Files - Where are control points?
- Index(es):
  - Chronological
  - Thread