[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: loop back connector

- To: <support@dieboldes.com>
- Subject: Re: loop back connector
- From: "Nel Finberg" <nel@dieboldes.com>
- Date: Tue, 17 Sep 2002 12:23:50 -0700
- References: <033b01c25e04$e6174500$18b8bfa8@LESLEY>

Lesley, the loopback connector is used in conjunction with the Main Serial Port Test in Diagnostics Mode on the AccuVote-OS. It is connected to the 9-pin COMM PORT connector at the back of the AccuVote-OS while the test is in progress, crossing pins 2 and 3, in order for outgoing transmissions to be received back over the same port. Nel ----- Original Message ----- From: Lesley Thompson (earthlink) To: support@dieboldes.com Sent: Monday, September 16, 2002 9:44 PM Subject: loop back connector What is a loop back connector and where do I get one? ______________________________________________________________________________________________________________ Lesley Koop Thompson Customer Service Project Manager Diebold Election Systems, Inc. 415-235-6553 (office cell) 512-413-7618 (cell) lesley@dieboldes.com

- Follow-Ups:
  - RE: loop back connector
    - From: "Ian S. Piper" <ian@dieboldes.com>

- References:
  - loop back connector
    - From: "Lesley Thompson \(earthlink\)" <lesleytdiebold@earthlink.net>

- Prev by Date: Re: date published request for staff site docs
- Next by Date: RE: loop back connector
- Index(es):
  - Chronological
  - Thread