[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: modem card for R6

- To: <support@gesn.com>
- Subject: Re: modem card for R6
- From: "Tari Runyan" <trglobal@earthlink.net>
- Date: Thu, 10 Jan 2002 18:23:36 -0700
- References: <00b301c19a37$ab965740$3c03a8c0@obrien>

this one is Win CE compatible but may need an adaptor - any thoughts ----- Original Message ----- From: Ian S. Piper To: support@gesn.com Sent: Thursday, January 10, 2002 5:34 PM Subject: RE: modem card for R6 Tari: Pardon me for the error. You can also find modems at the site. Ian S. Piper -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ken Clark Sent: January 10, 2002 6:20 PM To: support@gesn.com Subject: RE: modem card for R6 She was asking about modems. Ken -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ian S. Piper Sent: Thursday, January 10, 2002 4:12 PM To: support@gesn.com Subject: RE: modem card for R6 Tari: Todate, we've been using the Socket LP-E Ethernet card. The Xircom model you've mentioned requires drivers to be loaded. This site Windows CE 2.1 Compatible Peripherals lists compatible CE devices, but like the Xircom, most of them require drivers to be loaded. When you look at the list at the hyperlink above, I believe that those listed with the logo below, are compatible with the generic drivers already embedded in Windows CE 2.1. So they should be plug and pray. Due to availability issues and "obsolescence" (I'm learning to hate that word), you may be stuck having to use a Compact Flash Type with a PCMCIA Type II Adapter. This means that there would be two pieces to create what used to be one. So far, we've wanted to stay away from this combination format, due to the confusion that might result from poll workers inappropriately pulling at the cards installed in an R6 unit and finding the compact flash detaching from the PCMCIA Adapter. But that's probably not so much of a concern with the Ethernet cards, as poll workers won't be handling them. In case we're forced in this direction by the industry, are there any thoughts from the field support people on using the Compact Flash Type peripherals with the Adapter? Sincerely, Ian S. Piper -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Tari Runyan Sent: January 10, 2002 5:31 PM To: Support Subject: modem card for R6 would this modem card be good for what we need ? runs about $160

| Japanese | Contact us

Now you can send e-mails, browse the Internet from your Pocket PC...no string attached* !!
*Pretec's CompactModem is not a wireless/cellular modem. This modem does not require any dangle/cable for connecting from the card to the phone jack. However, it requires a regular phone line to connect from the built-in RJ-11C connector to the phone jack on the wall.
Pretec's CompactModemTM is the world's first and smallest 56Kbps Fax/Data Modem card for WindowsCE based Pocket PC and Handheld PC. Pretec's 56K Fax/Modem of Rockwell version is based on the K56flexTM and supporting ITU-T V.90 standard which delivers up to 56Kbps downloads utilizing ordinary analog phone line. This Fax/Modem Card also supports the V.80 application interface capable of operating with any H.324 Video Phone systems designed to provide affordable video conference over ordinary telephone lines. By adding one inexpensive CompactFlash adapter, the card becomes a full-fledged PC card - to be used with most notebook computers and instruments with PCMCIA slots. This card features low power consumption, and innovative power management resulting in battery life increase of your portable computers. It is the best choice for data communication requirements on your mobile computers.
For OEM/Industrial/Government/distribution customers, please sent your inquiry via this E-Mail Web form.
For evaluation sample or end-user sales, please visit our online store. |
Features CompactFlashTM sized package 3.3V low power consumption with power management: Auto sleep and wake-up Support ITU-T V.90 & K56flexTM Up to 56Kbps download data transmission 14,400bps send & receive Fax Plug-and-Play, Easy Installation, Hot swapping and card insertion V.42 and MNP 2-4 Error Correction V.42bis and MNP5 Data Compression Auto fall back down to 300bps auto-sync Asynchronous, full duplex V.80 and Rockwell Video Ready synchronous access modes support host-based communication protocols
Specifications Dimensions: CompactFlashTM Type I card: 36.4mm(L)* 42.8mm(W)*3.3mm(H) Type I card plus Extender: 49.2mm(L)*42.8mm(w)*15.78mm(H) Telephone interface: RJ-11C System Requirement: CompactFlash Slot or PCMCIA Type II slot PC 386 or higher with 4 MB RAM System Compatible: DOS, Windows 3.x, WIN95, WIN98, WINDOW CE, Window NT Newton MessagePad Operating Mode: Asynchronous data and fax modem Automatic or manual answer and origination Internal DAA for direct connection to Public Switched Telephone Networks Full-Duplex or Half-Duplex Tone or Pulse dialing mode Data Modem: ITU-T V.90 & K56flex: 56000bps down to 28800bps DTE interface: up to 115,200bps 33.6Kbps, 31.2Kbps, V.34, V.32bis,V.32, V.22bis, V.22A/B, V.23, and V.21;Bell 212A and 103 V.42 LAPM, MNP2-4, and MNP10 error correction V.42bis and MNP5 data compression MNP 10EC TMenhanced cellular performance Flow Control: Hardware (RTS/CTS) and Software (XON/XOFF) Speaker signal available to Host for call progress monitoring Fax Modem: Send and receive up to 14.4kbps ITU-T V.17, V.29, V.27ter, and V.21 channel 2 Voice Modem: Enhanced ADPCM Audio Span: ITU-T V.61 modulation(4.8 kbps data plus audio) Handset, headset, or half-duplex speakerphone ITU-T V.70 DSVD (option): : ITU-T interoperable G.729 and G.729 Annex A with interoperable G.729 Annex B SIG(special interest group) DigiTalk DSVD Voice/silence detection and handset echo cancellation Robust DSVD timing recovery Handset, headset, or half-duplex speakerphone Full-duplex Speakerphone(FDSP) Mode: Acoustic and line echo cancellation Microphone gain and muting Speaker volume control and muting Room monitor Modem Diagnostics: : Local analog lookback test, Local analog lookback with self-test, Local digital lookback test, Remote digital lookback with self-test Signaling: Adaptive Equalization: Receiver sensitivity : -43 dBm Transmit level : -10 dBm normal Dynamic range : 34 dB (between -9 ~ -43dBm) Power Management: Operating Voltage : 3.3V +/-5% Operating mode: 0.2W Typical Sleep mode: - User programmable inactivity timer for sleep mode - Wake up via Ring signal detection or any AT command Environment conditions: Operating temperature: 0 oC to 55oC Storage temperature: -20oC to 65oC Relative humidity: 95%(Max) Altitude: 20,000ft Agency Approvals: OFCC Part 15 and 68, PTT UL certified accessories

Copyright PRETEC 2000 /2001 | Legal information |

- Follow-Ups:
  - RE: modem card for R6
    - From: "Ian S. Piper" <ian@gesn.com>

- References:
  - RE: modem card for R6
    - From: "Ian S. Piper" <ian@gesn.com>

- Prev by Date: Re: modem card for R6
- Next by Date: RE: modem card for R6
- Index(es):
  - Chronological
  - Thread