[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: AVTS set IP address useability

- To: <bugtrack@dieboldes.com>
- Subject: Re: AVTS set IP address useability
- From: "Talbot Iredale" <tiredale@dieboldes.com>
- Date: Mon, 1 Apr 2002 09:57:58 -0800
- References: <000701c1cebd$2d0de270$2304a8c0@kclark>

This has now been fixed. You can now insert the manager card at the prompt for insertion of election media to access the setup screen. This will be in BallotStation 4.3.2. Tab ----- Original Message ----- From: Ken Clark To: bugtrack@dieboldes.com Sent: Monday, March 18, 2002 12:40 PM Subject: AVTS set IP address useability Scenario: receive an AVTS unit with serial number set up, but IP address not set up. Want to download a memory card via Ethernet. BS 4.3 and CE 3.0 provide functionality to set the IP address in setup. You can’t get to setup without a programmed memory card. You can’t download a memory card until you have networking setup. And so on. Ken

- Prev by Date: Re: Pennsylvania Cross-Endorse SOVC error
- Next by Date: gems 1-17-20 does not display any TS ballot images or vote centers
- Index(es):
  - Chronological
  - Thread