[Date Prev][Date Next] [Chronological] [Thread] [Top]

# AVTS set IP address useability

- To: <bugtrack@dieboldes.com>
- Subject: AVTS set IP address useability
- From: "Ken Clark" <ken@dieboldes.com>
- Date: Mon, 18 Mar 2002 12:40:43 -0800
- Importance: Normal

Scenario: receive an AVTS unit with serial number set up, but IP address not set up. Want to download a memory card via Ethernet. BS 4.3 and CE 3.0 provide functionality to set the IP address in setup. You can’t get to setup without a programmed memory card. You can’t download a memory card until you have networking setup. And so on. Ken

- Follow-Ups:
  - Re: AVTS set IP address useability
    - From: "Steve Knecht" <skglobal@earthlink.net>
  - RE: AVTS set IP address useability
    - From: "Jeff Hallmark" <jeffh@dieboldes.com>

- Prev by Date: RE: Spyrus units going down -March 2002
- Next by Date: Re: AVTS set IP address useability
- Index(es):
  - Chronological
  - Thread