[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: Installation procedure for Ethernet card (Socket LPE) in R6

- To: <support@gesn.com>
- Subject: RE: Installation procedure for Ethernet card (Socket LPE) in R6
- From: "Jeff Hallmark" <jeffh@gesn.com>
- Date: Thu, 17 Jan 2002 17:14:44 -0600
- Importance: Normal
- In-reply-to: <022001c19fa8$2ae57f10$3c03a8c0@obrien>

No, the only restriction I am aware of , as you know, is that CE images must be loaded via the lower slot.
Any other configuration for example, loading a new version of Ballot Station or for downloading election media,
is at the sole discretion of the user.
It does seem that to download successive election media on one unit, multiple pcmcia card insertion / removals, that one
would want the ethernet card in the lower slot and the most often removed media in the upper slot.
Short answer is , no, it isn't the only slot that will work.
Jeff Hallmark

> -----Original Message-----
> From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ian S. Piper
> Sent: Thursday, January 17, 2002 4:42 PM
> To: support@gesn.com
> Subject: RE: Installation procedure for Ethernet card (Socket LPE) in R6
> Jeff:
> You indicate to install the network card in the top slot. Is that the only slot that will work?
> Sincerely,
> Ian S. Piper
> -----Original Message-----
> From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Jeff Hallmark
> Sent: January 17, 2002 4:16 PM
> To: support
> Subject: Installation procedure for ethernet card (Socket LPE) in R6

> > Find attached word doc with install procedure.

- References:
  - RE: Installation procedure for Ethernet card (Socket LPE) in R6
    - From: "Ian S. Piper" <ian@gesn.com>

- Prev by Date: RE: Installation procedure for ethernet card (Socket LPE) in R6
- Next by Date: RE: Installation procedure for ethernet card (Socket LPE) in R6
- Index(es):
  - Chronological
  - Thread