[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: R6 Power status

- To: <support@gesn.com>
- Subject: Re: R6 Power status
- From: "Talbot Iredale" <tiredale@gesn.com>
- Date: Tue, 5 Jun 2001 12:47:02 -0700
- References: <LPEMLNDEKOMBOFJGLHCJAEBBCGAA.tyler@gesn.com>

    The battery statuses displayed are those that are defined by the Win32 API.
    In theory on the R6 unit you should never see the "Unknown" status. On the
    R4 unit, since there is not power management system installed, you will
    always see "Unknown" as the power status.

    As for the other statuses:
    "High"     - battery level is high (ie well charged)
    "Low"     - battery level is low (ie not well charged)
    "Critical"  - battery level is critically low and the system will shut down
    soon
    "Charging" - battery is charging
    "No Battery" - there is no battery.

    Currently the system is not very good at determining the status of the
    battery. In particular the R6 unit will only detect charging, high and low
    conditions.

    Tab

    ----- Original Message -----
    From: "Tyler Lincks" <tyler@gesn.com>
    To: <support@gesn.com>
    Sent: Tuesday, June 05, 2001 12:34 PM
    Subject: RE: R6 Power status

    > No, it all pretty much makes sense to me now.  I am assuming that a power
    > status of "low" or "critical" only appears if the unit is running off
    > battery power (or unless...there's a comeback editorial comment hanging
    out
    > there, but I can't say it without making someone angry).
    >
    > Tyler
    >
    > -----Original Message-----
    > From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of
    > Ken Clark
    > Sent: Tuesday, June 05, 2001 2:04 PM
    > To: support@gesn.com
    > Subject: RE: R6 Power status
    >
    >
    > > From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of
    > > Tyler Lincks
    > > Sent: Tuesday, June 05, 2001 12:05 PM
    > >
    > > Ergo if the unit has a battery and is plugged in, its power status
    should
    > > always be "high" (battery fully charged) or "charging", nez pas?
    >
    > You'd think so.  I am assuming you are going to get to the part where you
    > tell us its not eventually, right?
    >
    > > And what
    > > would cause the unit to be unable to discern the status of the
    > > battery (i.e.
    > > "unknown")?
    >
    > There is an internal sensor that determines whether Steve Knecht is in the
    > room, and that status is displayed in this case.
    >
    > You are right.  That state doesn't make sense to me either, and if it
    does,
    > the cases where it can happen should be documented.
    >
    > Ken

- References:
  - RE: R6 Power status
    - From: "Tyler Lincks" <tyler@gesn.com>

- Prev by Date: RE: R6 Power status
- Next by Date: RE: GEMS V1.17.11.1 & AccuVote 1.96.1 - Blank Ballots Report
- Index(es):
  - Chronological
  - Thread