[Date Prev][Date Next] [Chronological] [Thread] [Top]

# AV Server 1 COM Ports

- To: support@gesn.com
- Subject: AV Server 1 COM Ports
- From: Mark S Earley <meglobal@earthlink.net>
- Date: Fri, 4 Jan 2002 16:36:01 -0500

    While performing test uploads from AVOS units to AV Server 1, COM Ports
    do not reset until AVOS unit is powered OFF or port is cycled thru
    STOP/START. Is this normal, or is there some setting that can correct
    this?

    I found that setting modem S register S19=1 will put the COM Port back
    to "Waiting For Call" status after 1 minute. Is there any hidden problem
    with this?

    Mark
    Mark S Earley
    Support Services Specialist
    Global Election Systems
    office: 850 422-2100
    cell: 850 322-3226

- Follow-Ups:
  - Re: AV Server 1 COM Ports
    - From: "Steve Knecht" <skglobal@earthlink.net>

- Prev by Date: Re: Sacramento demo database
- Next by Date: Re: AV Server 1 COM Ports
- Index(es):
  - Chronological
  - Thread