[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: BallotStation 4-1-3 NT touch screen calibration

- To: <bugtrack@dieboldes.com>
- Subject: Re: BallotStation 4-1-3 NT touch screen calibration
- From: "Talbot Iredale" <tiredale@dieboldes.com>
- Date: Thu, 13 Dec 2001 09:57:52 -0800
- References: <003601c1745c$13160cf0$0a04a8c0@dieboldes.com>

This is fixed and will be in the next 4.2 release Tab ----- Original Message ----- From: Nel Finberg To: Bug Track Sent: Friday, November 23, 2001 12:18 PM Subject: BallotStation 4-1-3 NT touch screen calibration Clicking on the Calibrate TS button in the System Setup window in BallotStation 4-1-3 NT causes the following error message to be displayed: Nel

- Prev by Date: CMR 1-0-1 will load keys but doesn't hold them
- Next by Date: Re: VCProgrammer-3.13.5.1 - Error message when creating a voter card after it has been voted on the AVTS
- Index(es):
  - Chronological
  - Thread