[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: AVTS set IP address useability

- To: <bugtrack@dieboldes.com>
- Subject: RE: AVTS set IP address useability
- From: "Jeff Hallmark" <jeffh@dieboldes.com>
- Date: Mon, 18 Mar 2002 17:18:37 -0600
- Importance: Normal
- In-reply-to: <000701c1cebd$2d0de270$2304a8c0@kclark>

DHCP, the default setting for networking, has been tested, well for one connection, here in McKinney using (Socket LPE ethernet and CE 3.0) Jeff Hallmark -----Original Message----- From: owner-bugtrack@dieboldes.com [mailto:owner-bugtrack@dieboldes.com]On Behalf Of Ken Clark Sent: Monday, March 18, 2002 2:41 PM To: bugtrack@dieboldes.com Subject: AVTS set IP address useability Scenario: receive an AVTS unit with serial number set up, but IP address not set up. Want to download a memory card via Ethernet. BS 4.3 and CE 3.0 provide functionality to set the IP address in setup. You can’t get to setup without a programmed memory card. You can’t download a memory card until you have networking setup. And so on. Ken

- References:
  - AVTS set IP address useability
    - From: "Ken Clark" <ken@dieboldes.com>

- Prev by Date: Re: AVTS set IP address useability
- Next by Date: Recalled candidate name(s) playing after unvoted Recall Race
- Index(es):
  - Chronological
  - Thread