[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: AV Server 1 COM Ports

- To: <support@gesn.com>
- Subject: Re: AV Server 1 COM Ports
- From: "Steve Knecht" <skglobal@earthlink.net>
- Date: Fri, 4 Jan 2002 17:53:46 -0800
- References: <2.1-15816-573-A-OEWW@mail.earthlink.net>

    Mark,
    As far as I know that sounds like the "common behavior".  That is the modem
    in the field does not "hang up" until they power off the AccuVote in the
    field.   Whether there are better methods or not I don't know, but that is
    what we "train" for.
    ----- Original Message -----
    From: Mark S Earley <meglobal@earthlink.net>
    To: <support@gesn.com>
    Sent: Friday, January 04, 2002 1:36 PM
    Subject: AV Server 1 COM Ports

    > While performing test uploads from AVOS units to AV Server 1, COM Ports
    > do not reset until AVOS unit is powered OFF or port is cycled thru
    > STOP/START. Is this normal, or is there some setting that can correct
    > this?
    >
    > I found that setting modem S register S19=1 will put the COM Port back
    > to "Waiting For Call" status after 1 minute. Is there any hidden problem
    > with this?
    >
    > Mark
    > Mark S Earley
    > Support Services Specialist
    > Global Election Systems
    > office: 850 422-2100
    > cell: 850 322-3226
    >

- Follow-Ups:
  - Re: AV Server 1 COM Ports
    - From: Mark S Earley <meglobal@earthlink.net>

- References:
  - AV Server 1 COM Ports
    - From: Mark S Earley <meglobal@earthlink.net>

- Prev by Date: AV Server 1 COM Ports
- Next by Date: Re: AV Server 1 COM Ports
- Index(es):
  - Chronological
  - Thread