[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: Touch Screen Calibration with BS Software

- To: <rcr@dieboldes.com>
- Subject: RE: Touch Screen Calibration with BS Software
- From: "Ian S. Piper" <ian@dieboldes.com>
- Date: Thu, 25 Oct 2001 09:41:49 -0500
- Importance: Normal
- In-Reply-To: <PPECJKNKLDJLKJPKPPIOOEPEDCAA.ken@dieboldes.com>

-----Original Message----- From: owner-rcr@dieboldes.com [mailto:owner-rcr@dieboldes.com]On Behalf Of Ken Clark they use the proceedure I described: double entry. If you screw up twice, you are deemed too stupid to own a palm pilot. Then you remove the batteries and get factory defaults, and start over. Good Luck. I hope it flies. But if it doesn't, there's always "WD-40". That'll always get us out of a sticky situation. Ian

- References:
  - RE: Touch Screen Calibration with BS Software
    - From: "Ken Clark" <ken@dieboldes.com>

- Prev by Date: Re: Touch Screen Calibration with BS Software
- Next by Date: BS Audit Log - Challenge Accept Notation
- Index(es):
  - Chronological
  - Thread