[Date Prev][Date Next] [Chronological] [Thread] [Top]

# PLEASE REVIEW & COMMENT: JoCoKs AVOS Central Count Scanner Diagonstics Checklist

- To: <support@gesn.com>
- Subject: PLEASE REVIEW & COMMENT: JoCoKs AVOS Central Count Scanner Diagonstics Checklist
- From: "Lesley Thompson" <lesleytdiebold@earthlink.net>
- Date: Tue, 16 Jul 2002 14:50:01 -0500
- Organization: Diebold Election Systems, Inc.

Dear fellow support staff, below is Johnson County's current checklist for AVOS scanner diagnostics prior to central count. I need this reviewed to make sure it includes all the diagnostic type items that need to be tested. Thanks in advance for any and all help granted. Lesley Lesley Koop Thompson Customer Service Project Manager Diebold Election Systems, Inc. lesley@dieboldes.com OR lesleytdiebold@earthlink.net 512-413-7618 (cell) 415-235-6553 (DESI cell)
Election Date: | Scanner Number:
JoCoKs Scanner Diagnostics Checklist – AccuVote-OS Central Count
Night Before
| Turn on scanner to charge battery – leave on overnight
# Test Day
| Turn scanner off
| Check that printer has sufficient paper – Replace paper roll with AccuVote off
| Turn on Feeder
| Hold down Y & N buttons while turning AccuVote on Release when display comes up Scanner is now in Diagnostics Mode
| # Test Network? – Y
| · Set Baud rate to 9600? – N
| · Set Baud rate to 19200? – Y
| Logging In Message
| Connecting Message
| · Echo Connection Test? – N
| · Test Network – N
| # Test LCD Display? – Y
| · Test Continuous? – N
| # Test System Memory? - Y
| · Test Continuous? – N
| Test Printer? UNPLUG power from AccuVote and Feeder, then – Y (Low Power message will flash while unplugged – this is OK)
| · Repeat Test – Y (total of 3 tests)
| Check tape for legible output
| Plug power back in
| · Repeat Test – N
| # Test Main Serial Port? – N
| # Test Auxiliary Serial Port? – N
| Test Ballot Deflector? – N
| Test Ballot Reader – Y
| · Test with Auto feeder? – Y
| Insert Diagnostic Ballot in Reader – run card through four times – on the 5th time, hold down Y to get report
| · Turn ballot over & repeat on other side
| (Each report will show number of ballots read, length = 41, % of values – look for 100% and 0% on each test)
| Turn AccuVote and Feeder OFF
| Check for sufficient paper – replace if necessary
| Replace ribbon if necessary
Tested by: | Date:

- Follow-Ups:
  - RE: PLEASE REVIEW & COMMENT: JoCoKs AVOS Central Count Scanner Diagonstics Checklist
    - From: "Ian S. Piper" <ian@dieboldes.com>

- Prev by Date: RE: password request
- Next by Date: RE: bugzilla down, we are working on it
- Index(es):
  - Chronological
  - Thread