[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: How to restore if PCMCIA goes south

- To: <support@gesn.com>
- Subject: RE: How to restore if PCMCIA goes south
- From: "Sophia Lee" <sophia@gesn.com>
- Date: Fri, 25 Jan 2002 15:36:56 -0800
- Importance: Normal
- In-reply-to: <002401c1a5f1$c397a040$0e03a8c0@globalow6zn1fu>

Greg, Here's what you do if your PCMCIA card goes SOUTH: 1. Download another PCMCIA card for the same vote center. 2. Put that PCMCIA card into election mode. 3. Go into Supervisor Mode. 4. End the election. 5. Select "Election Archives". 6. Select "Current Election" Loc=Main from the "Elections" window. 6. Touch "All Directories" and "All Machines". 7. Select the archive to restore from. 8. Touch "Restore". 9. Touch "Done". 10. Touch "Resume Count". I think. -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Greg Forsythe Sent: Friday, January 25, 2002 2:44 PM To: support@gesn.com Subject: Re: How to restore if PCMCIA goes south Hi Jeff, Email down all day. Do you have the passcode for the AccuVote-TS Users guide? Greg ----- Original Message ----- From: Jeff Hintz To: support@gesn.com Sent: Friday, January 25, 2002 10:03 AM Subject: RE: How to restore if PCMCIA goes south Look at section 11.11.3, (Restoring an Election), of the AccuVote-TS User’s Guide. Jeff -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Greg Forsythe Sent: Thursday, January 24, 2002 8:38 PM To: Support Subject: How to restore if PCMCIA goes south If the PCMCIA card is lost for whatever reason, is there any way to recreate a new one from the originating Ballot Station? Greg Forsythe Diebold Election Systems (416) 446-1383 office (416) 446-1425 fax (416) 464-3736 cell www.gesn.com

- Follow-Ups:
  - Re: How to restore if PCMCIA goes south
    - From: "Greg Forsythe" <gfglobal@earthlink.net>

- References:
  - Re: How to restore if PCMCIA goes south
    - From: "Greg Forsythe" <gfglobal@earthlink.net>

- Prev by Date: Re: How to restore if PCMCIA goes south
- Next by Date: Re: R6 modem testing successful
- Index(es):
  - Chronological
  - Thread