[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Power Supply Requirements

- To: "Tab Iredale" <tab@gesn.com>
- Subject: Power Supply Requirements
- From: "Juan Rivera" <juan@gesn.com>
- Date: Thu, 28 Jan 1999 09:54:28 -0600
- Cc: "Support" <support@gesn.com>

    I am Resending this info just in case that the original message was lost...

    +12 Volts DC
                        1.5 Amps to 2.0 Amps  when Idel
                        3.5 Amps to 4.0 Amps  surged

    + 5 Volts DC
                        3.5 Amps to 4.0 Amps  when Idel
                        6.5 Amps to 7.0 Amps  surged

    -12 Volts and - 5 Volts DC are the same

                        .5 Amps to .75 Amps     when Idel
                        .75 Amps to 1.0 Amps   surged

- Prev by Date: Gaston's ABC Referendum Dates
- Next by Date: Upgrade from 1.3.3 to 1.5.2
- Index(es):
  - Chronological
  - Thread