[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Cleaning cloths for AV-TS Units

- To: <support@gesn.com>
- Subject: Cleaning cloths for AV-TS Units
- From: "Ian S. Piper" <ian@gesn.com>
- Date: Wed, 2 Aug 2000 14:45:48 -0500
- Importance: Normal

    I would like to clarify the recommended cleaning cloth to be used on all
    AV-TS Unit Touch Panel surfaces.

    It is available from Wal-Mart Optical Departments.  Ask for a "Lens Cleaning
    Cloth with Microfibres".  Also identified by Wal-Mart's part number
    K-788-SWB.  It approximately eight (8) inches square and comes in a variety
    of colors.

    They're approximately $1.50 each and they are reuseable for quite a number
    of units.  How many units depends on how dirty the AV-TS unit touch panels
    are when you clean them.  These cloths remove fingerprints and smudges from
    the touch panel surface without effort.  These cloths do not have abrasive
    fibres and are not impregnated with chemicals.  Do not wash them in an
    attempt to extend their life.  Buy a new one.

    It is recommended that they be used dry.   Do not use them with a liquid
    (e.g., isopropanol, ammonia).  Liquid solvents and glass cleaners will cause
    the laminates of the touch panel to separate.

    Again, I stress to not use any liquids (e.g., isopropanol, Windex, etc.) on
    the touch panel surface or its surrounding bezel.

    I recommend that all support staff involved with AV-TS units pick up a
    couple of these items to have on hand.  Global will only purchase these
    cloths for production purposes.  We will not stock them.

    Sincerely,

    Ian S. Piper
    Manufacturing Manager
    Global Election Systems, Inc.

- Follow-Ups:
  - AVTS power usage
    - From: "Robert Chen" <rcglobal@earthlink.net>
  - RE: Cleaning cloths for AV-TS Units
    - From: "Ken Clark" <ken@gesn.com>
  - Re: Cleaning cloths for AV-TS Units
    - From: "Greg Forsythe" <gfglobal@earthlink.net>

- Prev by Date: Re: Official Options For Withdrawn Candidates?
- Next by Date: AVTS power usage
- Index(es):
  - Chronological
  - Thread