[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: AV Server 1 COM Ports

- To: <support@gesn.com>
- Subject: Re: AV Server 1 COM Ports
- From: "Steve Knecht" <skglobal@earthlink.net>
- Date: Sat, 5 Jan 2002 11:59:28 -0800
- References: <2.1-15816-573-A-OEWW@mail.earthlink.net> <5.1.0.14.0.20020104211350.00aafad0@mail.earthlink.net>

    That's a question for someone more technical than I.  I'm sure someone else
    can respond to this.
    ----- Original Message -----
    From: Mark S Earley <meglobal@earthlink.net>
    To: <support@gesn.com>
    Sent: Friday, January 04, 2002 6:31 PM
    Subject: Re: AV Server 1 COM Ports

    > Thanks Steve. Somehow I never picked up on that before.
    >
    > Any problems with setting the S19 register to 1? This resets the modem to
    > Waiting For Call after 1 minute of inactivity. I tried it and it works
    > better than leaving the line hanging indefinitely.
    >
    > I'm a little worried it may interfere with some kind of delayed up or down
    > load, or modem usage outside of GEMS.
    >
    > Mark
    > At 1/4/2002 08:53 PM, you wrote:
    > >Mark,
    > >As far as I know that sounds like the "common behavior".  That is the
    modem
    > >in the field does not "hang up" until they power off the AccuVote in the
    > >field.   Whether there are better methods or not I don't know, but that
    is
    > >what we "train" for.
    > >----- Original Message -----
    > >From: Mark S Earley <meglobal@earthlink.net>
    > >To: <support@gesn.com>
    > >Sent: Friday, January 04, 2002 1:36 PM
    > >Subject: AV Server 1 COM Ports
    > >
    > >
    > > > While performing test uploads from AVOS units to AV Server 1, COM
    Ports
    > > > do not reset until AVOS unit is powered OFF or port is cycled thru
    > > > STOP/START. Is this normal, or is there some setting that can correct
    > > > this?
    > > >
    > > > I found that setting modem S register S19=1 will put the COM Port back
    > > > to "Waiting For Call" status after 1 minute. Is there any hidden
    problem
    > > > with this?
    > > >
    > > > Mark
    > > > Mark S Earley
    > > > Support Services Specialist
    > > > Global Election Systems
    > > > office: 850 422-2100
    > > > cell: 850 322-3226
    > > >
    >
    >

- Follow-Ups:
  - Re: AV Server 1 COM Ports
    - From: Ken Clark <kwclark71@yahoo.com>

- References:
  - AV Server 1 COM Ports
    - From: Mark S Earley <meglobal@earthlink.net>
  - Re: AV Server 1 COM Ports
    - From: Mark S Earley <meglobal@earthlink.net>

- Prev by Date: Re: AV Server 1 COM Ports
- Next by Date: Report to show cards exceeding selected ballot length
- Index(es):
  - Chronological
  - Thread