[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: Ballot Station 4.1.0.2 boot with voter card inserted

- To: <bugtrack@dieboldes.com>
- Subject: Re: Ballot Station 4.1.0.2 boot with voter card inserted
- From: "Nel Finberg" <nel@dieboldes.com>
- Date: Tue, 11 Sep 2001 12:52:35 -0700
- References: <009301c13703$a093b9b0$0a04a8c0@dieboldes.com> <002701c13af9$23511a70$1404a8c0@dieboldes.com>

This problem still occurs in BallotStation 4.1.0.4. Nel ----- Original Message ----- From: Talbot Iredale To: bugtrack@dieboldes.com Sent: Tuesday, September 11, 2001 12:37 PM Subject: Re: Ballot Station 4.1.0.2 boot with voter card inserted This problem exists in 4.0.9 and 4.1.0.2. It is now fixed and will be in 4.0.10 and 4.1.0.3. Tab ----- Original Message ----- From: Nel Finberg To: Bug Track Sent: Thursday, September 06, 2001 11:42 AM Subject: Ballot Station 4.1.0.2 boot with voter card inserted Booting the AccuVote-TS R6 with a voter card inserted into the card reader causes the message 'Remove unknown card from reader' to appear on the Ballot Station desktop. After removal of the voter card, however, the message does not disappear. It is necessary to reboot the unit. Nel

- Follow-Ups:
  - RE: Ballot Station 4.1.0.2 boot with voter card inserted
    - From: "Ken Clark" <ken@dieboldes.com>

- References:
  - Ballot Station 4.1.0.2 boot with voter card inserted
    - From: "Nel Finberg" <nel@dieboldes.com>
  - Re: Ballot Station 4.1.0.2 boot with voter card inserted
    - From: "Talbot Iredale" <tiredale@dieboldes.com>

- Prev by Date: Re: Ballot Station 4.1.0.2 boot with voter card inserted
- Next by Date: RE: Ballot Station 4.1.0.2 boot with voter card inserted
- Index(es):
  - Chronological
  - Thread