[Date Prev][Date Next] [Chronological] [Thread] [Top]

# AVTS modem upload BS 4.3.11

- To: <support@gesn.com>
- Subject: AVTS modem upload BS 4.3.11
- From: "Robert Chen" <robertc@dieboldes.com>
- Date: Mon, 28 Oct 2002 13:30:46 -0800
- Importance: Normal

    Hi,

    Found something interesting here in Alameda County, and want to see if
    anyone has found this in the field.  Especially those of you who are doing
    AVTS (we don't do AVOS) modem upload from the precincts.

    Running:
    BS 4.3.11
    GEMS 1.18.14
    NT 4.0 6a

    I am dialing the central computer's bank of modems (connected via Digi PCI
    X/em) and connecting to NT's Remote Access Server.  I have assigned a ip
    pool (166.107.248.210 to 220) and the AVTS with PCMCIA card modems dial in
    okay, and make a connection with the RAS server.  I can see the assigned ip
    address to the incoming AVTS unit.  However, when I try uploading, it gives
    and error: "no connection to host".  Yes, I have confirmed the HOST name and
    tried the IP address.

    I tried pinging the AVTS unit and only get timeouts.  I then tried
    simulating the connection with my laptop and was able to successfully
    upload.  I was also able to ping my laptop from the server and vice versa.

    At this point, I do not think, despite the port information displayed by RAS
    Server, that the AVTS was taking the ip address.

    I am sure I am probably doing something wrong and would appreciate some
    enlightenment.

    rob chen

- Follow-Ups:
  - Re: AVTS modem upload BS 4.3.11
    - From: "Talbot Iredale" <tiredale@dieboldes.com>

- Prev by Date: RE: auto l and a on TS unit doesn't populate all precincts
- Next by Date: Re: AVTS modem upload BS 4.3.11
- Index(es):
  - Chronological
  - Thread