[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: AV-TS R6 Battery Charge Indication

- To: <support@gesn.com>
- Subject: RE: AV-TS R6 Battery Charge Indication
- From: "Ken Clark" <ken@gesn.com>
- Date: Tue, 28 May 2002 14:16:57 -0800
- Importance: Normal
- In-reply-to: <OEEDJDHNNOPPJKLNFFFLMEFCCDAA.josh@gesn.com>

This will appear in Ballot Station 4.3.7 and 4.4.1. Hats off to Ataa for hitting the keys on this project. Ken -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com] On Behalf Of Josh Gardner Sent: Tuesday, May 28, 2002 1:09 PM To: support@gesn.com Subject: FW: AV-TS R6 Battery Charge Indication -----Original Message----- From: owner-devel@gesn.com [mailto:owner-devel@gesn.com]On Behalf Of Ataa A. El-Ganayni Sent: May 28, 2002 13:34 To: devel@gesn.com Subject: RE: AV-TS R6 Battery Charge Indication Enclosed is a screen shot of one of the states Battery Power Indicator can represent. Power Indicator represents two main things: 1- AC Power (Online / Offline.) 2- Battery Charging percentage. When AC power is offline, the indicator background is always red, regardless of the battery charging condition. Otherwise, the background of the battery percentage will be red when battery is below 40%, yellow from 40% to 99% and green for 100%. Ataa El-Ganayni

- References:
  - FW: AV-TS R6 Battery Charge Indication
    - From: "Josh Gardner" <josh@gesn.com>

- Prev by Date: FW: AV-TS R6 Battery Charge Indication
- Next by Date: RE: test
- Index(es):
  - Chronological
  - Thread