[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: WCE 300 - July 05, 2002 Release

- To: <support@dieboldes.com>
- Subject: RE: WCE 300 - July 05, 2002 Release
- From: "Steve Knecht" <stevek@dieboldes.com>
- Date: Tue, 6 Aug 2002 14:17:06 -0700
- Importance: Normal
- In-reply-to: <621FD3E588CC1B47A560B16C666D403943B0DA@msexch15.diebold.com>

Thanks. -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Green, Pat Sent: Tuesday, August 06, 2002 11:02 AM To: 'support@dieboldes.com' Subject: RE: WCE 300 - July 05, 2002 Release Steve, It was believed that only units built for Georgia would be affected. However, Lesley had 38 units shipped to Johnson County around the same time, so she was affected as well. There should be no others (famous last words). Older units with CE 2.12 never had the problem, so there was only a week or so of problem units leaving the factory. Pat -----Original Message----- From: Steve Knecht [mailto:stevek@dieboldes.com] Sent: Tuesday, August 06, 2002 1:36 PM To: support@dieboldes.com Subject: RE: WCE 300 - July 05, 2002 Release At what point does manufacturing (what point in delivery to which sites) did this get caught. Is it corrected in shipments to accounts today. What accounts do we need to check on this? -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ian S. Piper Sent: Tuesday, August 06, 2002 6:47 AM To: support@dieboldes.com Subject: RE: WCE 300 - July 05, 2002 Release I believe the password you have is only for the July 5th edition of WinCE and not the Clock Fix Utility. Try the password in the info directly below. <ClockFix Utility Information> This program (nk.bin) is loaded from the PCMCIA card by the boot loader and then initializes the PIC's RTC. The program does not get copied to the internal Flash therefore there is no need to re-load the WinCE image after running the clock fix program. If a valid date already exists then the date will not be modified. The ClockFix program is on the ftp site under the BS4Fix directory. It is called ClockFix.zip and password is "and83jd92ndjs". Unzip the file and copy it to a PCMCIA card, then insert the card into the bottom PCMCIA slot and turn the AVTS unit on. It will display a message that it is fixing the clock and then when it is done it will tell the user to turn to unit off. <End of ClockFix Info> -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Lesley Thompson Sent: Monday, August 05, 2002 11:02 PM To: support@gesn.com Subject: Fw: WCE 300 - July 05, 2002 Release Greg, this one worked for me. Lesley ----- Original Message ----- From: Talbot Iredale To: Software Announcements Sent: Friday, July 05, 2002 2:23 PM Subject: WCE 300 - July 05, 2002 Release The July 4, 2002 release did not update the release date. This is fixed in the July 05, 2000 release which is now on the ftp site. The password is "njdks893ndj12" Tab

- References:
  - RE: WCE 300 - July 05, 2002 Release
    - From: "Green, Pat" <GreenP@diebold.com>

- Prev by Date: Re: Can GEMS 1.17.22 run on Win2000 with one AVOS?
- Next by Date: RE: Can GEMS 1.17.22 run on Win2000 with one AVOS?
- Index(es):
  - Chronological
  - Thread