[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: R6 Power status

- To: <support@gesn.com>
- Subject: RE: R6 Power status
- From: "Ian S. Piper" <ian@gesn.com>
- Date: Tue, 5 Jun 2001 13:47:51 -0500
- Importance: Normal
- In-reply-to: <LPEMLNDEKOMBOFJGLHCJKEAOCGAA.tyler@gesn.com>

    You don't have to power the unit up to charge the battery.  All you need do
    is plug the unit into AC Power.  The R6 battery charging system does the
    rest.

    Ian

    -----Original Message-----
    From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of
    Tyler Lincks
    Sent: June 05, 2001 1:42 PM
    To: support@gesn.com
    Subject: RE: R6 Power status

    OK smart aleck, does the battery charge any time the unit is plugged in and
    turned on?  (Yes, your honor, I am leading the witness...)

    Tyler

    -----Original Message-----
    From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of
    Ken Clark
    Sent: Tuesday, June 05, 2001 11:44 AM
    To: support@gesn.com
    Subject: RE: R6 Power status

    > From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of
    > Tyler Lincks
    >
    > The "Power" field on the R6 election mode screen can (according to the R6
    > User's Guide) be defined as high,

    The charge in the battery is high.

    > low,

    The charge in the battery is low.

    > critical,

    The charge in the battery is critically low.

    > charging,

    The battery is charging.

    > no battery,

    There is no battery.

    > and
    > unknown.

    The state of the battery isn't known.

    > What does each of these mean?

    That's why they pay us the big bucks, to explain these things.

    Ken

- Follow-Ups:
  - RE: R6 Power status
    - From: "Tyler Lincks" <tyler@gesn.com>

- References:
  - RE: R6 Power status
    - From: "Tyler Lincks" <tyler@gesn.com>

- Prev by Date: RE: R6 Power status
- Next by Date: RE: R6 Power status
- Index(es):
  - Chronological
  - Thread