[Date Prev][Date Next] [Chronological] [Thread] [Top]

# restoring a bad pcmcia card

- To: <support@dieboldes.com>
- Subject: restoring a bad pcmcia card
- From: "Tari Runyan" <tarir@dieboldes.com>
- Date: Wed, 23 Oct 2002 09:35:06 -0600
- Organization: Diebold Election Systems

this is from El Paso who had this happen and worked with Jeff Hallmark and our restore directions the Correct solution is : Active Election Machine - Storage device (pcmcia card) goes bad. To resolve.... Download SAME Machine memory card from GEMS - note new copy # Start TS with NO memory card in place. Insert Managers Card - enter Supervisor Functions DELETE THE ELECTION! - this step actually makes a copy in the Archives to be restored from (scary step). Insert new memory card, go to Election Archives Select appropriate election on the top pane - location must be main, must be an archived election. Check boxes to show all directories, all machines Select from below the appropriate election.brs file that has results, click restore. Click okay twice (two warning messages pop up). Verify that totals match old card Lock up card until ready to transmit results - card can no longer be voted on. Tari

- Follow-Ups:
  - RE: restoring a bad pcmcia card
    - From: "Jeff Hallmark" <jeffh@dieboldes.com>
  - Re: restoring a bad pcmcia card
    - From: "Talbot Iredale" <tiredale@dieboldes.com>

- Prev by Date: RE: Election Support Document
- Next by Date: RE: restoring a bad pcmcia card
- Index(es):
  - Chronological
  - Thread