[Date Prev][Date Next] [Chronological] [Thread] [Top]

# modem card for R6

- To: "Support" <support@gesn.com>
- Subject: modem card for R6
- From: "Tari Runyan" <trglobal@earthlink.net>
- Date: Thu, 10 Jan 2002 16:30:45 -0700

would this modem card be good for what we need ? runs about $160

Xircom CompactCard Modem 56 GlobalACCESS for Windows CE
Description: Xircom CompactCard Modem 56 GlobalACCESS for Windows CE, includes one CompactCard Modem 56 GlobalACCESS, modem cable connector and telephone cord. CompactCards, CompactFlash cards for Windows CE access email, browse the Internet, and rapidly synchronize and exchange data between Windows CE handheld devices and Windows-based PCs.
Manufacturer: XIRCOM | Mfr. Model: CFM56G
UPC code: 093888024527 | Category: MODEMS
Technical Notes: 0 | Weight: .5 lb.
Bus/Port Type: CompactCard | Cellular Capability: Yes
Data Transfer Rate: 56 Kbps | Ethernet Included: No
Platform: Windows CE | Technology: V.90 & K56Flex compatible
Model: CFM56G Description: XIRCOM CompactCard Modem 56 GlobalACCESS Features: CompactFlash Card-size 56Kbps Modem w/ GlobalACCESS gives Windows CE users high-speed 56K modem access, enabling you to rapidly synchronize, communicate, and exchange information worldwide. Access a wide variety of online resources, including e-mail and the Internet, conveniently from your Windows CE handheld using a standard 56K connection. This low-power CompactCard features BatterySave™ advanced power management, ensuring longer handheld battery life when the CompactCard is not in use. A member of the Xircom family of GlobalACCESS™ products, the CompactCard Modem 56 GlobalACCESS is the ideal anywhere, anytime 56K access solution for your Windows CE handheld. Interface: CompactFash card-size with PC Card Type II adapter Connectors: (1) RJ11 modem connector Data Modulation: V.90/K56flex up to 56,000bps V.34 up to 33600bps; V.32terbo at 19200 and 16800 bps V.32bis at 14400, 12000, 9600, 7200 bps, uncoded at 4800 V.32 at 9600 bps uncoded at 4800 bps V.22bis at 2400 bps, V.22 at 1200 bps V.23 at 1200, 75 bps, Bell 212A at 1200 bps. Fax Modulation: V.17 at 14000, 12000, 9600, 7200 and 4800 bps. V.29 at 9600, 8200 and 4800 bps. V.27ter at 4800 and 2400 bps. Fax Support: Group 3, EIA/TIA; Class 1 and Class 2 Error Control: V.42/MNP levels 2-4 Compression: Data: V.42bis (4:1) or MNP Level 5 (2:1) Command Set: Hayes, Microcom compatible AT commands. Memory: 4 Megabits of memory accommodates dual-mode operation for V.90 and K56flex Ram: Non-volatile: 1 user-definable profile; up to 2 thirty-six digit telephone numbers and serial number. LEDs: Carrier detect (green), Transmission activity (yellow) Compatibility: Supports handhelds using MIPS 3000, MIPS 4000, Hitachi SH3, Hitachi SH4, and StrongARM processors. Approvals: FCC-B, CE Mark, UL Requirements: designed for Windows CE 1.1 or higher; supports synchronization from Microsoft Windows 95/98/NT 4.0/2000. Power: Active 180mA @ 3.3 volts, Idle 18mA @ 3.3 volts Size: 1.63" x 1.69" x 0.20" Weight: 0.35 ounces Manufacturer Warranty: Lifetime; www.xircom.com Warranty and Support Lifetime warranty from manufacturer Tech support from PSI and respective manufacturers. PRICE Please click here. TO ORDER OR INQUIRE Please e-mail us at psi@psism.com or call (301) 572-2168 to order and/or inquire. We accept Visa, MasterCard, and American Express as well as government and university POs. International orders, POs, and COD payments are also accepted but may require additional fees. Please click here to place your order and view our ordering information page.
Notebook Enhancements | Memories | PCMCIA Cards/Readers | Digital Cameras & Cards | Router Memory Palmtop Memory Cards | Monster Monitors | USB & Firewire Products | Specialty Items | OEM Manufacturers PSI Home TronLink Home Copyright© 1995-2000 Primary Simulation, Inc. 2963 Mozart Drive, Silver Spring, MD 20904 U.S.A. (301) 572-2168, Fax: (301) 572-2169 email: psi@psism.com

- Follow-Ups:
  - RE: modem card for R6
    - From: "Ian S. Piper" <ian@gesn.com>

- Prev by Date: Re: Precinct check number on AVOS tape
- Next by Date: Extra results for Johnson County, KS mock election
- Index(es):
  - Chronological
  - Thread