[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: WCE 300 - July 05, 2002 Release

- To: <support@dieboldes.com>
- Subject: RE: WCE 300 - July 05, 2002 Release
- From: "Ian S. Piper" <ian@dieboldes.com>
- Date: Tue, 6 Aug 2002 13:02:24 -0500
- Importance: Normal
- In-reply-to: <NGBBJFAJENGBILFIMBGFKECBCEAA.stevek@dieboldes.com>

All production today has the Jul 5th edition WinCE with the Clock Fix Utility run on the unit. There were some units sent to Georgia that didn't have a valid time and date in the RTC as they were manufactured with the June 7th edition of WinCE and that edition couldn't set a time and date properly. These units are being upgraded to Jul 5th edition and the RTC corrected at the Atlanta Georgia warehouse as they are found. As all production at that time this occurred (mid to late June) had been directed to Georgia, I believe that Georgia is the only place that should experience this. Having said that, it may be that some units were redirected from Georgia shipments to accommodate priorities in other accounts. If the units in any of your accounts have Jul 5th edition WinCE and the unit displays "No battery" in the lower right corner then your first assumption would be to run the Clock Fix Utility. I wouldn't even bother to check the battery connections until this utility was run first. -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Steve Knecht Sent: Tuesday, August 06, 2002 12:36 PM To: support@dieboldes.com Subject: RE: WCE 300 - July 05, 2002 Release At what point does manufacturing (what point in delivery to which sites) did this get caught. Is it corrected in shipments to accounts today. What accounts do we need to check on this? -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ian S. Piper Sent: Tuesday, August 06, 2002 6:47 AM To: support@dieboldes.com Subject: RE: WCE 300 - July 05, 2002 Release I believe the password you have is only for the July 5th edition of WinCE and not the Clock Fix Utility. Try the password in the info directly below. <ClockFix Utility Information> This program (nk.bin) is loaded from the PCMCIA card by the boot loader and then initializes the PIC's RTC. The program does not get copied to the internal Flash therefore there is no need to re-load the WinCE image after running the clock fix program. If a valid date already exists then the date will not be modified. The ClockFix program is on the ftp site under the BS4Fix directory. It is called ClockFix.zip and password is "and83jd92ndjs". Unzip the file and copy it to a PCMCIA card, then insert the card into the bottom PCMCIA slot and turn the AVTS unit on. It will display a message that it is fixing the clock and then when it is done it will tell the user to turn to unit off. <End of ClockFix Info> -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Lesley Thompson Sent: Monday, August 05, 2002 11:02 PM To: support@gesn.com Subject: Fw: WCE 300 - July 05, 2002 Release Greg, this one worked for me. Lesley ----- Original Message ----- From: Talbot Iredale To: Software Announcements Sent: Friday, July 05, 2002 2:23 PM Subject: WCE 300 - July 05, 2002 Release The July 4, 2002 release did not update the release date. This is fixed in the July 05, 2000 release which is now on the ftp site. The password is "njdks893ndj12" Tab

- References:
  - RE: WCE 300 - July 05, 2002 Release
    - From: "Steve Knecht" <stevek@dieboldes.com>

- Prev by Date: RE: WCE 300 - July 05, 2002 Release
- Next by Date: RE: WCE 300 - July 05, 2002 Release
- Index(es):
  - Chronological
  - Thread