[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: Modem Upload Problems

- To: <bugtrack@dieboldes.com>
- Subject: RE: Modem Upload Problems
- From: "Ken Clark" <ken@dieboldes.com>
- Date: Thu, 13 Jan 2000 13:54:18 -0600
- Importance: Normal
- In-reply-to: <009001bf5c85$216ef9b0$109db3d1@stevek.dieboldes.com>

This process occurs when the AccuVote is not turned off after the modem upload. It will cease if the AccuVote is turned off. So your pollworker instructions need to emphasize turning of AccuVote after modem upload. Or you need to reset the modem. This was experience from Marin. Steve No, the problem we are seeing is worse than this. It happens sometimes even if the AccuVote is turned off. I am going to implement Steve's timeout RCR for 1.15. This will hangup the modem even if the AV is not turned off. Ken

- Follow-Ups:
  - Re: Modem Upload Problems
    - From: Guy Lancaster <glanca@dieboldes.com>

- References:
  - Re: Modem Upload Problems
    - From: "Steve Knecht" <skglobal@earthlink.net>

- Prev by Date: Re: column order on print artwork scrren
- Next by Date: Re: column order on print artwork scrren
- Index(es):
  - Chronological
  - Thread