[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: Error: Failed to Initialize CBallotDLG

- To: <support@gesn.com>
- Subject: RE: Error: Failed to Initialize CBallotDLG
- From: "Ken Clark" <ken@gesn.com>
- Date: Tue, 21 Aug 2001 10:10:30 -0700
- Importance: Normal
- In-reply-to: <000d01c12a61$cf6aecd0$12650a40@northman>

From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Greg Forsythe Sent: Tuesday, August 21, 2001 9:53 AM The AMO election is running in the Royal York Hotel as I type on 4.1.0.1 with the Canadian Flag. Results are expected at 2:00 pm Toronto time. I expect to put in the Manager Card and print totals, then upload the diskettes to GEMS, and then upload the Memory Card. Should I anticipate any problems? I wouldn't know. I have never put a manager card into a R4 unit running 4.1.0.1. Has anyone? If a Smart Card is put into the R4 upside down, it locks the screen with the prompt indicating that a card be upside down. Ctrl Alt Del with the keyboard to end task and reset. Happened about 6 or 7 times so far on the three R4s. This needs a bugtrack, and serious investigation. 4.1.0.2 is not the answer though. It is meant only for VIBS testing/demonstration. No, they are not VIBS units and that is probably the reason the prompt comes up. Yep. Ken

- References:
  - Re: Error: Failed to Initialize CBallotDLG
    - From: "Greg Forsythe" <gfglobal@earthlink.net>

- Prev by Date: Re: BallotStation4-0-8
- Next by Date: RE: BallotStation4-0-8
- Index(es):
  - Chronological
  - Thread