[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: Network Cards for R-6

- To: <support@gesn.com>
- Subject: Re: Network Cards for R-6
- From: "Nel Finberg" <nel@gesn.com>
- Date: Wed, 5 Dec 2001 12:39:24 -0800
- References: <014501c17dc7$f4a34830$3c03a8c0@obrien>

A valid gateway must be defined to the R6. If a the host computer is identified with a name rather than an IP address, a valid DNS server on the network must be identified to the R6, otherwise, the numeric IP address should be used. Re-insert the LPE card in order for the latest configuration to be recognized. Also, ping the R6 IP address from the GEMS host in order to verify that the R6 is recognized to the network. Nel ----- Original Message ----- From: Ian S. Piper To: support@gesn.com Sent: Wednesday, December 05, 2001 12:03 PM Subject: RE: Network Cards for R-6 Nel: I believe that Jeff Hintz is working with a version of BallotStation that gives him access to Control Panel, yet when defining the IP address, it still does not connect. He is using the brand of Ethernet card that was listed as a supported model (Socket LP-E). What does he have to do, other than the IP address definition, to allow it to function as it has in the past. -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Nel Finberg Sent: December 05, 2001 1:42 PM To: support Subject: Re: Network Cards for R-6 Contemporary versions of the BallotStation 4.x firmware do not support IP address definition, as the utility that should activate when a new network card is installed is immediately suppressed, and Control Panel cannot be accessed on the R6. With the release of WinCE 3.0, IP address definition on the BallotStation will be possible again. The only transmission means currently supported is serial, which requires running a null modem cable between the R6 and the PC and running RAS over the PC port. The AccuVote-TS R6 I am using was originally configured with a BallotStation version that allowed access to the Control Panel and thus the ability to define an IP address, so that I can transmit over local area network. A unit initially configured with a newer version of BallotStation, such as the one you are probably using, does not allow access to the Control Panel cannot be assigned an IP address, and therefore can only be used with a serial card. Nel ----- Original Message ----- From: Jeff Hintz To: 'Jeff Hallmark' Cc: Nel (E-mail) Sent: Wednesday, December 05, 2001 10:51 AM Subject: RE: Network Cards for R-6 I have received a LP-E ethernet card for the R-6. I have plugged it in, and even tried giving an IP address, but I do not get a connection when I try to download an election. The R-6 just sits there trying to get a connection, then it times out. I need to get this working before I go to Johnson County, KS tomorrow. Thanks, Jeff -----Original Message----- From: Jeff Hallmark [mailto:jeffh@gesn.com] Sent: Friday, November 30, 2001 9:33 AM To: Jeff Hintz Subject: RE: Network Cards for R-6 Jeff, The only ethernet card that has any run time here in McKinney is the "Socket" model LP-E. Visit their website http://www.socketcom.com/product/ethernet_card.htm. Install is fairly painless, be sure to run flush after you get it talking. jwh -----Original Message----- From: Jeff Hintz [mailto:jhglobal@earthlink.net] Sent: Thursday, November 29, 2001 3:38 PM To: Jeff Hallmark (E-mail); Nel (E-mail) Subject: Network Cards for R-6 Jeff & Nel, Johnson County, KS wants to do downloading and uploading via a Network Card. Is there only certain Network Cards that we can use, or can any PCMCIA Network Card be used??? Also, can you tell me the settings and installation for the Network Card. Thanks, JEFF HINTZ Global Election Systems

- References:
  - RE: Network Cards for R-6
    - From: "Ian S. Piper" <ian@gesn.com>

- Prev by Date: RE: Network Cards for R-6
- Next by Date: TS Open and Close Docs
- Index(es):
  - Chronological
  - Thread