[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: Ballot Station 4.3.6.1 Battery Charge indicator

- To: <bugtrack@gesn.com>
- Subject: RE: Ballot Station 4.3.6.1 Battery Charge indicator
- From: "Jeff Hallmark" <jeffh@gesn.com>
- Date: Wed, 29 May 2002 17:25:04 -0500
- Importance: Normal
- In-reply-to: <002801c20754$36effce0$3804a8c0@AGANAYNI>

For the following cases the AC power is always plugged in and power cycling between case 1 and case 2.
When there is a pcmcia card installed in the unit, programmed with an election, power on, the status of the battery is displayed as
case1 Charging green 80
When there is No pcmcia card installed in the unit, power on, administrator card inserted go into supervisor functions,the status of the battery is displayed as
case 2 AC Online green 100
Wait for communication cycle...then
case 3 Charging yellow 80
case 1 and case 2 should initialize with the same status.
case 1 and case 3 are inconsistent in colour as well.
Jeff Hallmark

> -----Original Message-----
> From: owner-bugtrack@gesn.com [mailto:owner-bugtrack@gesn.com]On Behalf Of Ataa A. El-Ganayni
> Sent: Wednesday, May 29, 2002 4:03 PM
> To: bugtrack@gesn.com
> Subject: RE: Ballot Station 4.3.6.1 Battery Charge indicator
> Would you please explain where is the bug here? Is it the change from 100% to 10% between the two dialog invocations?
> How much time was there between 1 and 2 below? and was the AC power cable unplugged before the second insertion of the admin card?
> Power status is updated approximately every one minute, so in-between changes will only show after the wait time elapses.
> Ataa El-Ganayni

> > -----Original Message-----
> > From: owner-bugtrack@gesn.com [mailto:owner-bugtrack@gesn.com] On Behalf Of Jeff Hallmark
> > Sent: Wednesday, May 29, 2002 1:06 PM
> > To: bugtrack
> > Subject: Ballot Station 4.3.6.1 Battery Charge indicator
> > On behalf of Don Vopalensky
> > No pcmcia installed
> > 1) admin card -> pin -> supervisor mode screen(Online/Battery green & 100)
> > 2) admin card -> pin -> supervisor mode screen(Charging/Battery red & 10)
> > STAYS IN STATE 2 until power cycled
> > Jeff Hallmark
> > jeffh@gesn.com
> > 972 542 6000 x157

- References:
  - RE: Ballot Station 4.3.6.1 Battery Charge indicator
    - From: "Ataa A. El-Ganayni" <ataa@dieboldes.com>

- Prev by Date: RE: Ballot Station 4.3.6.1 Battery Charge indicator
- Next by Date: RE: Ballot Station 4.3.6.1 Battery Charge indicator
- Index(es):
  - Chronological
  - Thread