[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: BallotStation 4-3-4 Election Mode ballot retention in Pre-Election Testing Mode

- To: <support@gesn.com>
- Subject: RE: BallotStation 4-3-4 Election Mode ballot retention in Pre-Election Testing Mode
- From: "Sue Page" <spdiebold@earthlink.net>
- Date: Sun, 19 May 2002 13:24:36 -0400
- Importance: Normal
- In-reply-to: <004801c1fdd9$1ec5e1e0$7ad6fc9e@default>

Given the problem with the Spyrus, Montgomery County, Maryland, is currently planning to use a TS unit for making voter cards, rather than the Spyrus. The other Counties want to to know how to do the conversion at the poll, as a back-up if all the Spyrus go down. Could someone please write procedures for using the TS unit as an encoder - setting it up in advance, and converting at the polls, with illustrations? (Maryland is 4.1.6) If these procedures are posted, we can all use them. This will give us all a solution that is uniform and "blessed" by our own experts. The comfort level of the customers is increased when "official procedures" are provided, and this keeps us from duplicating effort. Thanks! Sue -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Steve Knecht Sent: Friday, May 17, 2002 3:29 PM To: support@gesn.com Subject: Re: BallotStation 4-3-4 Election Mode ballot retension in Pre-Election Testing Mode Tab, If you clear the results on the TS unit, then are you going to implement the request that Tari asked for: allowing a pollworker to make voter cards on a unit (in case the Spyrus or PCC runs out of battery or doesn't work). We need a backup method to make cards in the precinct. Exiting election mode to access the "CREATE CARD" function is important, but NOT if you lose the ballots on the unit. Comments? ----- Original Message ----- From: Talbot Iredale To: support@gesn.com Sent: Thursday, May 16, 2002 2:15 PM Subject: Re: BallotStation 4-3-4 Election Mode ballot retension in Pre-Election Testing Mode No, this is not the intended behavior. When reseting the election to pre-election mode the results are ment to be "cleared". Tab ----- Original Message ----- From: Nel Finberg To: Support Sent: Wednesday, May 15, 2002 5:23 PM Subject: BallotStation 4-3-4 Election Mode ballot retension in Pre-Election Testing Mode # An election is reset to Pre-Election Testing Mode from Post-Election Mode. Ballots counted in Election Mode are displayed in Pre-Election Testing Mode View Ballots window. Is this intended behavior? # # Nel

- Follow-Ups:
  - Re: BallotStation 4-3-4 Election Mode ballot retention in Pre-Election Testing Mode
    - From: "Lesley Thompson" <lesleytdiebold@earthlink.net>

- References:
  - Re: BallotStation 4-3-4 Election Mode ballot retension in Pre-Election Testing Mode
    - From: "Steve Knecht" <stevek@gesn.com>

- Prev by Date: HP phasing out Jornada
- Next by Date: Re: BallotStation 4-3-4 Election Mode ballot retention in Pre-Election Testing Mode
- Index(es):
  - Chronological
  - Thread