[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: Ballot postscript file size

- To: <support@gesn.com>
- Subject: Re: Ballot postscript file size
- From: "Barry Herron" <bhglobal@earthlink.net>
- Date: Sat, 19 Feb 2000 15:43:36 -0600

Ken, Thanks for the input. I will discuss further with Crepeau. Barry -----Original Message----- From: Ken Clark <ken@gesn.com> To: support@gesn.com <support@gesn.com> Date: Saturday, February 19, 2000 2:32 PM Subject: RE: Ballot postscript file size Their question is: can the customer send them a ballot file to size rather than the ballot image size of 11 x 17 for an 8 1/2 x 11 ballot? If so, they can eliminate the interim processes and go directly to plate. GEMS outputs its ballot image using whatever printer settings it is given, so this should be possible. Just set the paper setting to 8.5/11 and tweak the print offsets -- much like printing BOD to the 5si. One question I have though is how do they deal with the cut marks? Typically print shops print on paper larger than 8.5/11 and then cut to size using these marks. If they are printing directly to 8.5/11 stock then make sure they are aware of our registration tolerances. If the answer is no, is there a bridge software solution between the GEMS postscript file and the image setter? Is any one else addressing this issue? They should also be able to do it with any DTP software that can manipulate postscript or pdf. Adobe Illustrator could probably do it, as might Ghostview like Greg suggests. A capable and competent print shop would know better than I which tools are best. Ken

- Prev by Date: Re: Ballot postscript file size
- Next by Date: Re: Accu-Votes failure in relation to temperature
- Index(es):
  - Chronological
  - Thread