[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: Burning PCMCIA cards with Laptop + Win 2000

- To: <bugtrack@dieboldes.com>
- Subject: Re: Burning PCMCIA cards with Laptop + Win 2000
- From: "Talbot Iredale" <tiredale@dieboldes.com>
- Date: Thu, 7 Jun 2001 14:08:02 -0700
- References: <DLEFJEOMANOIOFONALCGCECFCJAA.mike@dieboldes.com>

The ballotStation now does an explicit flush of the files at the end of download. This should fix the problem but I cannot test it since I do not have the ability to download to a PCMCIA card on WinNT nor Win2000. This will be in the BallotStation 4.1.1.1 pre-release and the BallotStation 4.0.2.3 pre-release. Tab ----- Original Message ----- From: Mike Brown To: Bugtrack@Gesn. Com Sent: Tuesday, June 05, 2001 9:06 AM Subject: Burning PCMCIA cards with Laptop + Win 2000 If I burn a PCMCIA card with WinNT 4.0, I can remove the card, and place it in an R6 unit and the DB will load. Problem with this setup is, I can only burn 1 card, since the OS crashes after that. NT does not do well with hot swapping anything. When I attempt the same procedure with a windows 2000 machine, I can theoretically hot swap the PCMCIA card, if I make sure I wait the required 10-20 seconds for the machine to realize that I pulled the card, and it issue's me a dialog box that informs me of this. I then have to click the OK button to acknowledge to the system that I know I have removed the card, then I can insert a new blank card to continue burning my PCMCIA cards. That is all fine and dandy, but another problem arises, after burning the PCMCIA card, I them proceed casually over to the R6 unit, and insert the card, I then get the Download Election Dialog box, not the loading election. I have looked at the contents of the PCMCIA card, and have not seen any differences. The election will not load, and yes, I have tried this a few times with the same results. Mike Mike Brown 1611 Wilmeth Road, McKinney, T.X. 75069 PH: 972.542.6000 FX: 972.542.6044

- References:
  - Burning PCMCIA cards with Laptop + Win 2000
    - From: "Mike Brown" <mike@dieboldes.com>

- Prev by Date: Re: R6 header problems and multiple ballot precinct lockout
- Next by Date: BallotStationCE-4-0-2-2: Reporting in Pre-election Test Mode: Internal Error.
- Index(es):
  - Chronological
  - Thread