[Date Prev][Date Next] [Chronological] [Thread] [Top]

# BOD Image Scaling in GEMS

- To: "Request for Change Report" <rcr@dieboldes.com>
- Subject: BOD Image Scaling in GEMS
- From: "Ian Piper" <ian@dieboldes.com>
- Date: Wed, 25 Aug 1999 19:56:24 -0500
- Cc: "Larry Ensminger" <larry@dieboldes.com>

Could you please add the following to the rcr list: The ability for GEMS to adjust the size and origin of a ballot's image on the printed output of a BOD laser printer (specifically a Minolta Pageworks 25). When testing the Minolta Pageworks 20 as a BOD solution, it was found that the ballot image size on the paper was 4% larger across its width than a 100% image. We need the scaling (magnification) of the ballot image across the paper to be within +/- 2% of the 100% size. I believe the issue could be solved by providing a method of scaling the ballot image size up or down (by inches or points, or whatever units) and also a method of relocating the origin point (bottom left corner) using the same units as the scaling method. This should only have to be done once per computer/printer configuration. I don't have an estimate for a date needed. Larry Ensminger would have to provide that information.

- Follow-Ups:
  - RE: BOD Image Scaling in GEMS
    - From: "Ken Clark" <ken@dieboldes.com>

- Prev by Date: RE: SOVC with totals flag for Poll, absentee, and Early Voting
- Next by Date: RE: BOD Image Scaling in GEMS
- Index(es):
  - Chronological
  - Thread