[Date Prev][Date Next] [Chronological] [Thread] [Top]

# BallotStation 4.0.11 download error

- To: "Bug Track" <bugtrack@dieboldes.com>
- Subject: BallotStation 4.0.11 download error
- From: "Nel Finberg" <nel@dieboldes.com>
- Date: Mon, 1 Oct 2001 12:14:40 -0700

Three instances of the same vote center (defined with multiple memory cards) are queued for downloading in GEMS 1-17-16 over a LAN connection. The first vote center downloads successfully. The OK button is touched on the BallotStation in response to the 'Transfer Completed' message. Following this message, If you wish to download another please insert another election media and press OK, otherwise press Done to continue is displayed. Done is touched. Please remove the election media then press Okay to continue or press Shutdown to shutdown is displayed. At this point, the programmed election media is removed from the R6 unit and a blank PCMCIA card is installed. The 'Download Election' box appears automatically, and the OK button is touched. The download progress bar appears momentarily, followed by Not enough storage is available to process this command at the same time as The specified network name is no longer available on the GEMS host. Click on the OK button in the GEMS error message, and touch OK in the BallotStation error message. Transfer Failed is displayed on the BallotStation. Touching OK re-displays the 'Download Election' box, and touching OK in this box re-displays the 'not enough storage' message. Since the first vote center/machine combination downloaded successfully to a 32MB PCMCIA card, the second vote center/machine ID download should not encounter a space problem downloading to a 32MB card. Nel

- Follow-Ups:
  - Re: BallotStation 4.0.11 download error
    - From: "Talbot Iredale" <tiredale@dieboldes.com>

- Prev by Date: Re: Central Count Decks not showing on reports
- Next by Date: R4s that won't print
- Index(es):
  - Chronological
  - Thread