[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Lockup after overvote override - 1.95d

- To: "Bugs" <bugtrack@dieboldes.com>
- Subject: Lockup after overvote override - 1.95d
- From: "Ian Piper" <ian@dieboldes.com>
- Date: Mon, 27 Mar 2000 13:01:30 -0600

I received a call from Bill Bowers of GBS. When over-riding an overvoted ballot, the AccuVote will: - Process the ballot - Eject the ballot out the exit - Display an LCD message "MEM CARD REMOVED /SYSTEM HALTED" - System is locked up. He is in Wisconsin and has experienced this problem in three different customer sites running 1.95d firmware. One of the AccuVote units was identified as SN 70445. It is an infra-red reader unit. The units used with the other two experiences are not known. The problem is intermittent. Bill Bowers found that, on the previously mentioned unit, it happened one time in four overrides. But it is repeatable. He claims this has just started happening after the firmware upgrades to 1.95d in Wisconsin. Ian

- Prev by Date: RE: Voter Group Header assignment for generation of separate ballots
- Next by Date: AVTS 3.12.5 - Cannot exit
- Index(es):
  - Chronological
  - Thread