[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: AVOS AccuBasic Reports - Use GEMS card numbers when downloaded from GEMS

- To: <rcr@dieboldes.com>
- Subject: Re: AVOS AccuBasic Reports - Use GEMS card numbers when downloaded from GEMS
- From: "Tari Runyan" <trglobal@earthlink.net>
- Date: Tue, 19 Jun 2001 17:26:50 -0600
- References: <3B2FCF0A.C06AE2C3@dieboldes.com> <3B2FDF65.A0EF509B@dieboldes.com>

I think it should be done before certification since VTS is going the way of the round file - IMHO and we have many hoops to jump through for certification - if it gets put off we just have to do it later - so why not now since we are in Wyle? anyone else agree? disagree? ----- Original Message ----- From: Guy Lancaster To: rcr@dieboldes.com Sent: Tuesday, June 19, 2001 5:25 PM Subject: Re: AVOS AccuBasic Reports - Use GEMS card numbers when downloaded from GEMS It turns out that "fixing" this WILL require a firmware change. The card number is formatted in the AccuBasic interpreter in the firmware rather than in the .abo files as I believed. Unfortunately we don't want to touch any more code than we absolutely need to at this point in our certification efforts and therefore this change will have to wait until after certification. We could of course "hack" an .abo file to work around this but it would be a temporary workaround and would probably be considered a billable request. Guy

- Follow-Ups:
  - RE: AVOS AccuBasic Reports - Use GEMS card numbers when downloaded from GEMS
    - From: "Larry Dix" <ljdglobal@dieboldes.com>

- References:
  - AVOS AccuBasic Reports - Use GEMS card numbers when downloaded from GEMS
    - From: Guy Lancaster <glanca@dieboldes.com>
  - Re: AVOS AccuBasic Reports - Use GEMS card numbers when downloaded from GEMS
    - From: Guy Lancaster <glanca@dieboldes.com>

- Prev by Date: Re: AVOS AccuBasic Reports - Use GEMS card numbers when downloaded from GEMS
- Next by Date: RE: AVOS AccuBasic Reports - Use GEMS card numbers when downloaded from GEMS
- Index(es):
  - Chronological
  - Thread